#
DRIVELINE/AXLES

BHE035025002W01

Item | Specification
--- | ---
MT | AT
FRONT AND REAR AXLES
Front axle | Maximum wheel bearing play | (mm {in}) | 0.05 {0.002}
Rear axle | Maximum wheel bearing play | (mm {in}) | 0.05 {0.002}
Drive shaft | Length (Air in boot at atmospheric pressure) | Left side | (mm {in}) | 792.6-802.6 {31.21-31.59} | 791.1-801.1 {31.15-31.53}
Right side | (mm {in}) | 832.6-842.6 {32.78-33.17} | 831.1-841.1 {32.71-33.11}
Differential | Pinion height | (mm {in}) | 0.038 {0.0015} or less
Drive pinion preload | (N·m {kgf·cm, in·lbf}) | 1.3-1.7 {14-17, 12-15}
Backlash of drive pinion and ring gear | Standard | 0.09-0.11 {0.0035-0.0043}
Minimum | 0.05 {0.0020} or more
(mm {in}) | Variance | 0.07 {0.0028} or less
Oil | Grade | API service GL-5
Viscosity | SAE 90
Capacity (Approx. quantity) | 1.2-1.4 {1.3-1.4, 1.1-1.2}
(L {US qt, Imp qt})
PROPELLER SHAFT
Runout | (mm {in}) | 0.4 {0.016}
Starting torque | (N·m {kgf·cm, in·lbf}) | 0.29-0.98 {3.0-10, 2.7-8.6}