#
ROTOR DISASSEMBLY

BHE011002000E06

1. Disassemble in the order indicated in the table.

1 | Cut-off seal
2 | Cut-off seal spring
3 | Outer oil seal (See Oil Seal Disassembly Note.)
4 | Outer O-ring (large radius)
5 | Outer oil seal spring (See Oil Seal Spring Disassembly Note.)
6 | Inner oil seal (See Oil Seal Disassembly Note.)
7 | Inner O-ring (small radius)
8 | Inner oil seal spring (See Oil Seal Spring Disassembly Note.)

## Oil Seal Disassembly Note

1. Remove the oil seal using the SST.

  Caution

  • Be sure to keep the removed oil seals separated according to their removal position.

## Oil Seal Spring Disassembly Note

  Caution

  • Be sure to keep the removed oil seal springs separated according to their removal positions.