#
CAR-NAVIGATION SYSTEM OUTLINE

BHE092066000T01

• A 7 inch wide, pop-up LCD (*TFT) has been adopted to improve marketability.

• A hybrid in car-navigation system and map-matching function has been adopted to improve accuracy of detection of the vehicle's position.

• A remote control with an infrared transmitter has been adopted to improve operational ability.

• The languages and voices available for use with the car-navigation unit include English, French, German, Dutch, Spanish, and Italian. However, the language used in this manual is in English only.

  *TFT :
Thin Film Transistor