#
GENERATOR INSPECTION

BHE011718300W02

  Caution

  • Do not apply direct battery positive voltage to the generator terminal D, otherwise it could cause damage to the internal parts (power transistor) of the generator.

## Generator warning light

1. Verify that the battery is fully charged.

2. Verify that the drive belt deflection/tension is within the specification. (See DRIVE BELT DEFLECTION/TENSION INSPECTION.)

3. With the ignition switch at ON, verify that the generator warning light illuminates.

  • If it does not illuminate, inspect the generator warning light and the wiring harness.

  – If the generator warning light and the wiring harness are normal, inspect the PCM.

4. Verify that the generator warning light turns off after the engine is started.

  • If it does not turn off, check if any one of the following DTCs in the on-board diagnostic system are displayed: P0112, P0113, P2502, P2503, P2504. (See DTC TABLE.)

## Generator

### Voltage

1. Verify that the battery is fully charged.

2. Verify that the drive belt deflection/tension is within the specification. (See DRIVE BELT DEFLECTION/TENSION INSPECTION.)

3. Turn off all electrical loads.

4. Start the engine and verify that the generator rotates smoothly without any noise while the engine is running.

5. Measure the voltage at each terminal using a tester.

Standard specification

Terminal | IG-ON (V) | Idle (V) [20°C {68 °F}]
--- | --- | ---
B | B+ | 13.0-15.0
P | Approx. 1.0 or less | Approx. 3.0-8.0
D | Approx. 0 | *

  * :
Turn the following electrical loads on and verify that the voltage reading increases.

  • Headlights
  • Blower motor
  • Rear window defroster

### Current

1. Verify that the battery is fully charged.

2. Verify that the drive belt deflection/tension is within the specification. (See DRIVE BELT DEFLECTION/TENSION INSPECTION.)

3. Disconnect the negative battery cable.

4. Connect a tester capable of reading 120 A or above between generator terminal B and the wiring harness.

5. Connect the negative battery cable.

6. Turn off all electrical loads.

7. Start the engine.

8. Increase engine speed from 2,000-2,500 rpm.

9. Turn the following electrical loads on and verify that the current reading increases.

  • Headlights
  • Blower motor
  • Rear window defroster

  Note

  • Current required for generating power varies with electrical loads applied.

Reference value

Current possible for power generation (differs according to load)

[Conditions] ambient temperature 20°C {68 °F}, voltage 13.0-15.0 V, engine warm

Engine speed (rpm) | Terminal B current (A)
--- | ---
1,000 | 0*-70
2,000 | 0*-97

  * :
The lower limit must be more than 0 A.