#
AIR FILTER INSPECTION

BHE071113988W02

1. Verify that there is no damage, excessive dirt or abnormal odor on the air filter.

  • If there is any malfunction, replace the air filter.

  Note

  • The air filter cannot be reused by cleaning it with water or compressed air.
  • Replace the air filter at the following interval, depending on operating conditions.

Destinations | Interval (year or km {mile})
--- | ---
Europe (L.H.D., R.H.D.) | 2 or 40,000 {25,000}
Australia | 1 or 20,000 {12,500}