#
DTC C1306

BHE040243000W30

DTC | C1306 | Steering angle sensor (abnormal initialization)
DETECTION CONDITION | • The steering angle sensor detects that the initialization procedure has not been performed.
POSSIBLE CAUSE | • The initialization procedure for the steering angle sensor has not been performed. • Steering angle sensor malfunction • The negative battery cable connector was disconnected previously.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY OTHER DTC HAS BEEN RECORDED • Has DTC C2778 also been stored? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | Go to the next step.
2 | VERIFY INITIALIZATION PROCEDURE. • Has the steering angle sensor initialization procedure been performed? | Yes | Go to the next step.
No | Perform the steering angle sensor initialization procedure, then go to the next step. (See STEERING ANGLE SENSOR INITIALIZATION PROCEDURE.)
3 | VERIFY DTC TROUBLESHOOTING COMPLETED • Clear the DTC from the memory. (See Clearing DTCs Procedures.) • Is the same DTC present? | Yes | Repeat the inspection from Step 1. If the malfunction occurs again, replace the steering angle sensor. (See STEERING ANGLE SENSOR REMOVAL/INSTALLATION.)
No | Go to the next step.
4 | VERIFY AFTER REPAIR PROCEDURE • Are any other DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | DTC troubleshooting completed.