#
PID/DATA MONITOR TABLE [MULTIPLEX COMMUNICATION SYSTEM]

BHE090255430W03

PID name (definition) | Condition | Specification | PID monitor module | Terminal
--- | --- | --- | --- | ---
ABS_MSG (Missing message from the DSC HU/CM) | Present | Circuit in the DSC HU/CM is normal. | Instrument cluster | • DSC HU/CM: H, I • Instrument cluster: 1J, 1L
Not Present | Circuit in the DSC HU/CM is disable.
TCM_MSG (Missing message from the TCM) | Present | Circuit in the TCM is normal. | • TCM: 1V, 1Y • Instrument cluster: 1J, 1L
Not Present | Circuit in the TCM is disable.
EPS_MSG (Missing message from the EPS control module) | Present | Circuit in the EPS control module is normal | • EPS control module: 2K, 2M • Instrument cluster: 1J, 1L
Not Present | Circuit in the EPS control module is disable
PCM_MSG (Missing message from the PCM) | Present | Circuit in the PCM is normal. | • PCM: 4S, 4V • Instrument cluster: 1J, 1L
Not Present | Circuit in the PCM is disable.