#
FRONT DOOR LOCK ACTUATOR INSPECTION

BHE091458490W03

## Door Lock Actuator

1. Apply battery positive voltage to the front door lock actuator terminals and inspect the operation of the front door lock actuator.

  • If not as specified, replace the front door lock actuator.

Actuator operation | Connection
--- | ---
B+ | GND
Lock | A (F) | C (D)
Double lock | A (F) | B (E)
Unlock | C and B (D and E) | A (F)

  ( ) :
RH

## Door Lock-link Switch

1. Inspect for continuity between the door lock-link switch terminals.

  • If not as specified, replace the front door lock actuator.

## Door Key Cylinder Switch

1. Disconnect the front door lock actuator connector.

2. Inspect for continuity between the door lock-link switch terminals.

  • If not as specified, replace the front door lock actuator.