#
SELECTOR LEVER STRUCTURE

BHE051446010T02

## M Range Switch

### Outline

  • The M range switch detects the selector lever in M range position and sends a manual mode request signal to the TCM.

1 | M range switch

### Operation

  • The M range switch is an ON/OFF type switch that turns on when the selector lever is shifted to the M range. It also remains on during up-shift and down-shift operations.

## Up Switch

### Outline

  • The up switch detects an up-shift operation in the M range and sends an up-shift request signal to the TCM.

1 | Up switch

### Operation

  • The up switch is an ON/OFF type switch that turns on when the selector lever is in the M range (+) side position.

## Down Switch

### Outline

  • The down switch detects a down-shift operation in the M range and sends a down-shift request signal to the TCM.

1 | Down switch

### Operation

  • The down switch is an ON/OFF type switch that turns on when the selector lever is in the M range (-) side position.