#
CALIPER (FRONT) DISASSEMBLY/ASSEMBLY

BHE041133990W01

1. Disassemble in the order indicated in the table.

1 | Bleeder cap
2 | Bleeder screw
3 | Bolt
4 | Sleeve
5 | Piston (See Piston Disassembly Note.)
6 | Dust seal
7 | Piston seal
8 | Caliper body

2. Assemble in the reverse order of disassembly.

## Piston Disassembly Note

  Caution

  • The piston could be damaged if blown out with great force. Blow the compressed air slowly to prevent the piston from suddenly popping out.

1. Insert a piece of wood in the caliper as shown in the figure, and then blow compressed air through the bleeder screw hole to remove the piston from the caliper body.