#
CLOCK SPRING REMOVAL/INSTALLATION

BHE081066123W01

  Caution

  • If the disc on the combination switch is deformed or has foreign material adhering to it, performance of the steering angle sensor may be reduced, causing abnormal operation. When handling the clock spring, be careful not to deform the disc and make sure there is no foreign material on it.

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module.

(See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Remove the steering wheel.

(See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

4. Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Clock spring. (See Clock Spring Installation Note.)

6. Install in the reverse order of removal.

7. Turn the ignition switch to the ON position.

8. Verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system.

## Clock Spring Installation Note

  Caution

  • If the clock spring is not adjusted, the spring wire in the clock spring could over-wind and break when the steering wheel is turned. Always adjust the clock spring after installing it.

1. Adjust the clock spring after installing it. (See CLOCK SPRING ADJUSTMENT.)