#
TIRE HOUSE TRIM REMOVAL/INSTALLATION

BHE091768750W01

1. Remove the rear seat. (See REAR SEAT REMOVAL/INSTALLATION.)

2. Remove the inner scuff plate. (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)

3. Partially peel back the seaming welt.

4. Pull the tire house trim outward and detach clips A and locator pins B.

5. Detach tabs C and remove the tire house trim.

6. Install in the reverse order of removal.