#
GENERAL PROCEDURES (FRONT AND REAR AXLES)

BHE031001018W01

## Wheel And Tire Installation

1. When installing the wheels and tires, tighten the wheel nuts in a criss-cross pattern to the following tightening torque.

  Tightening torque
  88-118 N·m {9.0-12.0 kgf·m, 65.0-87.0 ft·lbf}

## Connector Disconnection

1. Disconnect the negative battery cable before performing any work that requires handling of connectors.

## Suspension Links Removal/Installation

1. For the joint sections with rubber bushings, raise the vehicle using a lift, and then temporarily tighten the installation bolts and nuts. Lower the vehicle to the ground and tighten them completely with the specified torque.