#
TRANSMISSION CONTROL MODULE (TCM) OUTLINE

BHE051318901T03

• The TCM controls automatic transmission operations. The TCM outputs control signals to the transmission according to the signals from other sensors and/or switches.

• In driving mode, there are five mode selections: NORMAL, POWER, MANUAL, cold engine coolant temperature, and slope. The TCM automatically selects the proper mode according to driving condition.