#
CAR-NAVIGATION UNIT CONSTRUCTION

BHE092066902T02

## Structure

• The car-navigation unit is located in the glove compartment.

• An Eject button, to eject the DVD-ROM from the loading slot, is included in the unit.

• A gyro sensor which detects vehicle cornering angle is built into the unit.

1 | DVD-ROM loading slot
2 | DVD-ROM
3 | Eject button

## Terminal Layout and Signals

Terminal | Signals
--- | ---
16-pin connector
| 1A | GND
1B | B+
1C | -
1D | ACC
1E | PR front speaker input (-)
1F | Illumination (-)
1G | PR front speaker input (+)
1H | Vehicle speed
1I | PR front speaker output (-)
1J | Parking brake switch
1K | PR front speaker output (+)
1L | R-range
1M | Front speaker output (-)
1N | Front speaker output (+)
1O | Front speaker input (-)
1P | Front speaker input (+)

Terminal | Signals
--- | ---
24-pin connector
| 2A | -
2B | -
2C | -
2D | -
2E | -
2F | -
2G | -
2H | -
2I | -
2J | -
2K | -
2L | -
2M | -
2N | Monitor serial input
2O | Shield GND
2P | Monitor serial output
2Q | Shield GND
2R | Video (composite sync)
2S | -
2T | Video (B)
2U | Video GND
2V | Video (G)
2W | -
2X | Video (R)

Terminal | Signals
--- | ---
8-pin connector (for extended function)
| 3A | -
3B | Serial output
3C | -
3D | Serial input
3E | Power
3F | Reset
3G | B+
3H | GND

Terminal | Signal
--- | ---
1-pin connector
| 4A | GPS antenna input