#
HEADLIGHT CLEANER SYSTEM OPERATION

BHE091901052T08

## Auto-operation

• If the windshield washer switch is turned on when the ignition and headlight switches are at the ON position, the headlight cleaner motor operates.

• The headlight cleaner operates only one time for every five times the windshield washer switch is operated.

• If manual operation occurs within two to five times of the windshield washer switch being operated, the number count is reset. Also, if the headlight switch is turned to the OFF and then to the ON position, the count is reset when the windshield washer switch is turned on.

## Manual Operation

• If the windshield washer switch is turned on two consecutive times when the ignition and headlight switches are at the ON position, the headlight cleaner motor operates.

1 | Headlight relay
2 | Headlight
3 | Windshield wiper and washer switch
4 | Windshield washer switch
5 | INT relay
6 | Headlight cleaner relay
7 | Headlight switch
8 | Windshield washer motor
9 | Headlight cleaner motor

1 | Ignition
2 | Headlight switch
3 | Windshield washer switch
4 | Headlight cleaner relay
5 | ON
6 | OFF
7 | Double click (Reset)
8 | Reset
9 | 1ST
10 | 2ND-5TH
11 | 2ND
12 | 1 S or Less