#
POWER BRAKE UNIT REMOVAL/INSTALLATION

BHE041143800W02

1. For R.H.D., remove the air pump. (See SECONDARY AIR INJECTION (AIR) PUMP REMOVAL/INSTALLATION.)

2. Remove the master cylinder. (See MASTER CYLINDER REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. After installation, perform brake pedal inspection. (See BRAKE PEDAL INSPECTION.)

1 | Brake pipe (L.H.D.)
2 | Vacuum hose
3 | Snap pin
4 | Clevis pin
5 | Nut
6 | Power brake unit
7 | Gasket
8 | Fork
9 | Locknut