#
REAR SPOILER INSTALLATION

BHE091651960W02

  Note

  • Double-sided adhesive tape has already been attached to the new rear spoiler.

  Warning

  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

1. When installing a new rear spoiler, follow the procedure below:

  (1) Remove the adhesive remaining on the body using razor.
  (2) Remove any grease or dirt from the adhesion surface of the body.

2. When reusing the rear spoiler, follow the procedure below:

  (1) Remove the adhesive remaining on the rear spoiler and the body using a razor.
  (2) Remove any grease or dirt from the adhesion surface of the rear spoiler and the body.
  (3) Apply primer to the bonding area of the rear spoiler.
  (4) Attach double-sided adhesive tape to the rear spoiler as shown.

3. Peel off the backing of the double-sided adhesive tape.

4. Attach the clips and install the rear spoiler to the trunk lid.