#
SUPER-LSD CONSTRUCTION

BHE031427100T04

• Inside the super-LSD, taper rings that are fixed to the differential gear case have been placed between the differential gear case and the side gears. Additionally, a cone is provided around the outer surface of the side gear.

• Springs and retainers are positioned between the right and left side gears to provide initial torque to the taper rings.

1 | Pinion gear
2 | Side gear
3 | Cone
4 | Taper ring
5 | Retainer
6 | Spring