#
MAP LIGHT REMOVAL/INSTALLATION

BHE091801058W01

1. Disconnect the negative battery cable.

2. Remove the screws.

3. Remove the map light. (See Map Light Removal Note.)

4. Disconnect the connector.

5. Remove the socket, then remove the map light bulb.

6. Install in the reverse order of removal.

## Map Light Removal Note

1. Insert a tape-wrapped flathead screwdriver into the gap between the headliner and the map light.

2. Press the tab, and remove the map light.