#
FRONT DOOR UNIT REMOVAL/INSTALLATION

BHE091159970W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner garnish (See INNER GARNISH REMOVAL/INSTALLATION.)
  (2) Front door trim (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)
  (3) Front door glass (See FRONT DOOR GLASS REMOVAL/INSTALLATION.)
  (4) Front door speaker (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

3. Disconnect the door lock actuator connector.

4. Remove the front door wiring harness from the front door unit.

5. Remove screw A.

6. Remove screws B and the fastener.

7. Remove the front door unit.

8. Remove the following parts:

  • Front power window motor
  • Front power window regulator
  • Front door speaker amplifier

9. Install in the reverse order of removal.