#
TRANSMITTER BATTERY INSPECTION

BHE091400110W03

  Caution

  • Since the battery voltage does not drop fully if the button is pushed for only 4 seconds or less, it can not be properly examined to see whether it is good or bad. Always push the button for 5 seconds.

  Note

  • A correct measurement cannot be obtained if the battery temperature is low. Make sure the battery is at 18 °C {64 °F} or more for at least 30 minutes before reinspecting if a measurement value is under the standard voltage.

1. Remove the transmitter cover.

2. Apply the ohmmeter leads to the positions as indicated in the figure.

3. While pressing the battery as shown in the figure, press the LOCK and UNLOCK buttons on the transmitter at the same time to start measurement of the voltage.

4. Release the buttons after 5 seconds.

5. Verify that the minimum voltage is the standard voltage or more for 10 seconds after starting measurement.

  • If the voltage is under the standard voltage, replace the battery.

  Standard voltage
  2.7 V