#
FRONT BUCKLE SWITCH INSPECTION

BHE081157620W02

## Driver-Side

1. Disconnect the negative battery cable.

2. Disconnect the buckle switch connector.

3. Verify continuity as indicated in the table.

  • If not as indicated in the table, replace the front buckle.

Manual seat

Power seat

## Passenger-Side

1. Disconnect the negative battery cable.

2. Disconnect the buckle switch connector.

3. Verify continuity as indicated in the table.

  • If not as indicated in the table, replace the front buckle.