#
SELECTOR LEVER REMOVAL/INSTALLATION

BHE051446102W03

1. Remove the engine cover.

2. Remove the battery cover.

3. Disconnect the negative battery cable.

4. Remove the following parts.

  (1) Ashtray
  (See CONSOLE REMOVAL/INSTALLATION.)
  (2) Console
  (See CONSOLE REMOVAL/INSTALLATION.)
  (3) Glove compartment
  (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)
  (4) Side panel
  (See SIDE PANEL REMOVAL/INSTALLATION.)
  (5) Lower panel
  (See LOWER PANEL REMOVAL/INSTALLATION.)
  (6) Column cover
  (See COLUMN COVER REMOVAL/INSTALLATION.)
  (7) Driver-side air bag module
  (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)
  (8) Steering shaft
  (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)
  (9) Instrument cluster
  (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)
  (10) A-pillar trim
  (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (11) Dashboard
  (See DASHBOARD REMOVAL/INSTALLATION.)
  (12) SAS unit
  (See SAS UNIT REMOVAL/INSTALLATION.)
  (13) Exhaust pipe
  (See EXHAUST SYSTEM REMOVAL/INSTALLATION.)

5. Shift the selector lever to the P position.

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

8. After installation, carry out the shift lock inspection and key interlock inspection.

(See SHIFT LOCK INSPECTION.)

(See KEY INTERLOCK INSPECTION.)

1 | Manual shaft lever component (See Manual Shaft Lever Component Removal Note.) (See Manual Shaft Lever Component Installation Note.)
2 | Clip
3 | Shift knob
4 | Console panel
5 | Indicator component
6 | Clip
7 | Brake switch (See Brake Switch Installation Note.)
8 | Interlock cable (See Interlock Cable Installation Note.)
9 | Selector lever

## Manual Shaft Lever Component Removal Note

1. Mark the manual shaft lever component as shown in the figure.

2. Remove the manual shaft lever component installation nut.

## Interlock Cable Installation Note

1. Verify that the selector lever is in the P position.

2. With the slider pin pressed in, slide the lock unit to fix the lock unit hook into the bracket hole securely as shown in the figure.

  Caution

  • Allowing the interlock cable to be bent or twisted during installation can affect the lock unit operation.

3. Verify that the slider pin slides freely, and rotate the slider pin to release the lock.

4. Remove your hand from the slider pin and verify that the end of the slider pin interferes with the stopper rubber of the brake pedal.

5. From this position, push the slider pin and rotate to lock.

6. Connect the brake switch connector when the brake pedal has completely returned.

7. Install the interlock cable end onto the interlock link on the selector lever.

8. Fit the interlock cable in the U-groove in the selector lever base plate and install the clip.

  Caution

  • Applying a load to the interlock cable while pressing the lock piece in can affect the lock unit operation.

9. Press the interlock cable lock piece in until it is locked.

10. Remove the snap pin as shown in the figure.

11. Turn the ignition switch to the ACC position.

12. Install the interlock cable to the key cylinder.

13. Slide the outer casing to the key cylinder and insert the clip over the convex part of the outer casing.

14. After installation, carry out the shift lock inspection, interlock inspection and brake switch inspection.

(See SHIFT LOCK INSPECTION.)

(See KEY INTERLOCK INSPECTION.)

(See BRAKE SWITCH INSPECTION.)

## Manual Shaft Lever Component Installation Note

1. Align the mark of the manual shaft lever component as shown in the figure.

2. Install the manual shaft lever component installation nut.

  Tightening torque
  10.8-14.7 N·m
  {1.1-1.4 kgf·m, 8.0-10.8 ft·lbf}