#
INTAKE-AIR SYSTEM INSPECTION

BHE011301005W06

1. Perform the following intake-air system part inspections.

  Note

  • If there is improper installation or a malfunction of an intake-air system part, it could cause poor emission, low engine output, or rough idling.

## Air Hose Inspection

1. Visually inspect the following items:

  • If there is any abnormality, reinstall or replace the air hose.

  – Is there any looseness or disconnection of air hose and air cleaner cover connecting parts?
  – Is there any looseness or disconnection of air hose and throttle body connecting parts?
  – Is the hose correctly installed?
  – Are there any cracks or splits in the air hose?

## Hose Inspection

1. Refer to the intake-air system hose routing diagram and verify that the hoses are installed in the correct positions. (See INTAKE-AIR SYSTEM HOSE ROUTING DIAGRAM.)

  • If there is any abnormality, install in the correct position.

2. Verify that there is no crushing, cracks, or splits on the intake air hose.

  • If there is any abnormality, repair or replace the intake air hose.

## Fresh-air Duct Inspection

1. Remove the fresh air duct. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

2. Verify that there is no damage or peeling on the heat shield gasket for the fresh air duct.

  • If there is any abnormality, repair or replace the fresh air duct.

## Air Cleaner Insulator Inspection

1. Verify that the air cleaner insulator has been installed.

  • If it has not been installed, install an air cleaner insulator.