#
STARTING PROCEDURE FOR ON-BOARD DIAGNOSTIC TEST MODE

BHE090266900W01

  Note

  • All DTCs displayed in the on-board diagnostic test mode should be entered in the Audio Repair Order Form.

1. Turn the ignition switch to the ACC or ON position.

2. While pressing the POWER button, simultaneously press the AM button and the TAPE/MD button for 2 s or more.

1 | AM button
2 | TAPE/MD button
3 | SEEK button
4 | POWER button

  Note

  • If several DTCs are in the memory, they can be displayed using the SEEK button.

3. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.