#
HEAD IMPACT PAD REMOVAL/INSTALLATION

BHE09176852XW01

1. Remove the following parts:

  (1) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)
  (2) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (3) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (4) Inner scuff plate (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  (5) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (6) Rear pillar trim (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (7) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (8) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (9) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (10) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)
  (11) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

2. Remove the fastener. (Rear)

3. Pull the head impact pad outward and detach clips A and B. (Front)

4. Pull the head impact pad outward and detach clips B. (Rear)

5. Remove the head impact pad.

6. Install in the reverse order of removal.