#
POWER WINDOW SYSTEM OUTLINE

BHE091258000T01

• The following functions have been adopted for the driver's side.

  – Manual open/close function
  – Auto open function (driver's side)
  – Power-cut function (driver's side)
  – Automatic window return function
  – Two-step down function
  – IG OFF timer function
  – Fail-safe function

• The following functions have been adopted for the passenger's side.

  – Manual open/close function

• The P/W CM (power window control module) inside the power window main switch, which detects the door glass movement distance and direction based on pulse signals of the power window motor, controls the driver-side functions.