#
PROPELLER SHAFT INSPECTION

BHE031525002W06

## For Carbon-Fiber Propeller Shaft

  Caution

  • Replace the propeller shaft if it is dropped.
  • Handle the propeller shaft with care so that the pipe is not damaged from striking surrounding objects or other impacts.
  • Replace the propeller shaft if there is any chipping or warping of the pipe.
  • Protect the propeller shaft from damage and handle with careful attention when working.

1. Use a dial gauge to measure the runout of the propeller shaft at each position.

  • If it exceeds the maximum specification, replace the propeller shaft.

  Maximum runout
  0.4 mm {0.016 in}

2. Inspect the play and rotation of the joint by turning the universal joint in the directions shown by the arrows.

  Initial torque (Reference value)
  0.29-0.98 N·m
  {3.0-10 kgf·cm, 2.7-8.6 in·lbf}

  • If there is any play or excessive initial torque, replace the propeller shaft.

3. Verify that the propeller shaft has no bends or damage.

  • If there is any malfunction, replace the propeller shaft.

4. Verify that there is a gap between the pipe and yoke flange.

  • If there is any malfunction, replace the propeller shaft.

5. Verify that there is no cracking, peeling or similar damage to the seal (where the pipe and yoke connect).

  • If there is any malfunction, replace the propeller shaft.

For Steel Propeller Shaft

1. Use a dial gauge to measure the runout of the propeller shaft at each position.

  • If it exceeds the maximum specification, replace the propeller shaft.

  Maximum runout
  0.4 mm {0.016 in}

2. Inspect the play and rotation of the joint by turning the universal joint in the direction shown by the arrow.

  Initial torque (Reference value)
  0.29-0.98 N·m
  {3.0-10 kgf·cm, 2.7-8.6 in·lbf}

  • If there is excessive play or initial torque, replace the propeller shaft.