FRONT SUSPENSION > General Description
COMPONENT
1. FRONT SUSPENSION

(1) | Spacer crossmember front | (15) | Stud bolt∗ | Tightening torque: N·m (kgf-m, ft-lb)
(2) | Crossmember COMPL front | (16) | Bushing rear front arm | T1: | 25 (2.5, 18.4)
(3) | Flange bolt | (17) | Bushing arm front | T2: | 39 (4.0, 28.8)
(4) | Self-locking nut A | (18) | Arm COMPL front | T3: | 50 (5.1, 36.9)
(5) | Stiffener | (19) | Ball joint COMPL | T4: | 60 (6.1, 44.3)
(6) | Bolt | (20) | Castle nut | T5: | 70 (7.1, 51.6)
(7) | Crossmember support front | (21) | Cotter pin | T6: | 95 (9.7, 70.1)
(8) | Stabilizer front | (22) | Front arm rear plate | T7: | 110 (11.2, 81.1)
(9) | Bushing stabilizer front | (23) | Self-locking nut B | T8: | 150 (15.3, 110.6)
(10) | Clamp stabilizer | (24) | Strut ASSY | T9: | 155 (15.8, 114.3)
(11) | Flange nut | (25) | Adjusting bolt
(12) | Stabilizer link front | (26) | Adjusting washer
(13) | Crossmember support rear | (27) | Front axle housing
(14) | Stopper arm front
∗: Cannot be reused if the stud bolt is removed from the vehicle.

2. FRONT STRUT

(1) | Dust seal | (6) | Dust cover front | Tightening torque: N·m (kgf-m, ft-lb)
(2) | Self-locking nut | (7) | Coil spring front | T1: | 32 (3.3, 23.6)
(3) | Flange nut | (8) | Helper front | T2: | 55 (5.6, 40.6)
(4) | Mount strut front | (9) | Rubber seat LWR |  |
(5) | Mount bearing front | (10) | Strut COMPL front |  |