ENTERTAINMENT & MONITORING
ETM

ENTERTAINMENT & MONITORING > General Description
LOCATION
1. AUDIO AND NAVIGATION SYSTEM

(1) | Speaker ASSY tweeter LH | (3) | Speaker ASSY tweeter RH | (5) | Audio ASSY or navigation ASSY
(2) | GPS antenna ASSY | (4) | Satellite switch ASSY |  |

(1) | Antenna ASSY roof | (4) | Power amplifier ASSY | (6) | Speaker ASSY woofer
(2) | Speaker ASSY front LH | (5) | Speaker ASSY rear RH | (7) | Speaker ASSY rear LH
(3) | Speaker ASSY front RH |  |  |  |

2. TELEMATICS SYSTEM

For locations, refer to “LOCATION” of “TELEMATICS SYSTEM (DIAGNOSTICS)” section. TELEMATICS SYSTEM (DIAGNOSTICS)>Electrical Component Location>LOCATION

ENTERTAINMENT & MONITORING > General Description
COMPONENT
1. DATA COMMUNICATION MODULE

(1) | Cap screw | (4) | Backup battery | Tightening torque: N·m (kgf-m, ft-lb)
(2) | Battery cover | (5) | Data communication module body | T: | 0.3 (0.03, 0.2)
(3) | Circlip |  |  |  |

ENTERTAINMENT & MONITORING > General Description
CAUTION

- When performing service operation, refer to “Repair Contents” in “General Description”. REPAIR CONTENTS>Repair Contents

- Before disconnecting connectors of sensors or units, be sure to disconnect the ground terminal from the battery sensor. When replacing the audio and MFD parts provided with memory functions, record the memory contents before disconnecting the ground terminal from the battery sensor.

- Be careful of the following items. Failing to do so may cause the airbag system malfunction.

  - Yellow connectors and harnesses with yellow tapes around them are the connectors and harnesses for the airbag system. When using a tester on these circuits, follow the cautions of “AIRBAG SYSTEM”. AIRBAG SYSTEM>General Description>CAUTION

  - Be careful not to damage the airbag system wiring harness when servicing the electrical parts around the steering column.

- When removing, installing or replacing the VDCCM&H/U, VDCCM&H/U bracket, steering wheel or steering angle sensor (steering roll connector), perform “VSC(VDC) Centering Mode” of the VDC. VEHICLE DYNAMICS CONTROL (VDC)>VDC Control Module and Hydraulic Control Unit (VDCCM&H/U)>ADJUSTMENT > VDC SENSOR MIDPOINT SETTING MODE

ENTERTAINMENT & MONITORING > General Description
PREPARATION TOOL
1. SPECIAL TOOL

ILLUSTRATION | TOOL NUMBER | DESCRIPTION | REMARKS
| — | SUBARU SELECT MONITOR 4 | Used for setting of each function and troubleshooting for electrical system. For detailed operation procedures, refer to “Help” of application.

2. GENERAL TOOL

DESCRIPTION | REMARKS
Circuit tester | Used for measuring resistance, voltage and current.
DST-i | Used together with Subaru Select Monitor 4.
Clip remover | Used for removing clips.

ENTERTAINMENT & MONITORING > Relay and Fuse
LOCATION

Main fuse box (M/B) | Fuse 20 A (power amplifier) | (A)
Fuse 10 A (data communication module∗1) | (B)
Fuse & relay box (F/B) | Fuse 20 A (front accessory power supply socket, rear accessory power supply socket (luggage room)) | (C)
Fuse 15 A (rear accessory power supply socket (console)) | (D)
Fuse 15 A (audio, navigation unit, power amplifier, external connection terminal (instrument panel / console), data communication module∗1) | (E)
Fuse 15 A (data communication module∗1) | (F)
Fuse 7.5 A (audio, navigation unit) | (G)

∗1: Model with telematics

For other related fuses, refer to the wiring diagram. WIRING SYSTEM>Power Supply Circuit>WIRING DIAGRAM

ENTERTAINMENT & MONITORING > Relay and Fuse
INSPECTION
1. CHECK FUSE
1.

Remove the fuse and inspect visually.

2.

If the fuse is blown out, replace the fuse.

If the fuse is blown again, check the system wiring harness.

ENTERTAINMENT & MONITORING > Audio System
WIRING DIAGRAM

Refer to “Audio and Navigation System” in the wiring diagram. WIRING SYSTEM>Audio and Navigation System>WIRING DIAGRAM

ENTERTAINMENT & MONITORING > Audio System
INSPECTION
1. BASIC INSPECTION

For basic inspection, refer to “Basic Diagnostic Procedure” in “INFOTAINMENT SYSTEM (DIAGNOSTICS)”. INFOTAINMENT(DIAGNOSTICS) >Basic Diagnostic Procedure

2. SYSTEM BLOCK DIAGRAM

For system block diagram, refer to “System Block Diagram” in “INFOTAINMENT SYSTEM (DIAGNOSTICS)”. INFOTAINMENT(DIAGNOSTICS) >General Description>SYSTEM BLOCK DIAGRAM

3. MODULE I/O SIGNAL

For the specification (electrical component), refer to “Control Module I/O Signal” of “INFOTAINMENT SYSTEM (DIAGNOSTICS)”. INFOTAINMENT(DIAGNOSTICS) >Control Module I/O Signal>ELECTRICAL SPECIFICATION

ENTERTAINMENT & MONITORING > Audio System
OPERATION
1. CHECK CONNECTIONS WITH LINE DIAG MODE
1.

Turn the ignition switch to ACC.

2.

Press the button (b) twice with the button (a) pressed.

Pressing the button (a) for 3 seconds or more, or turning the ignition switch from the OFF to ACC position can exit the diagnostic mode.

3.

{Line Diag} screen is displayed.

4.

Check the connection status with the {Connection} in the {Line Diag} screen.

Item | Contents | Inspection
GPS | GPS antenna connection | Check that the display shows OK. (Models with GPS antenna only)
MIC | MIC connection | If the display shows OK, check that the microphone input level in the {Microphone} item varies depending on the sound and voice.
Rr_CAM | Rr CAM Video signal | Check that the display shows OK.
AUX | AUX connection | Connect the pin jack for check into the AUX terminal, and check that the display shows OK.
USB1 | USB connection | Connect the memory for check into the USB terminal, and check that the display shows OK.
USB2 | USB connection (DCM) | Check that the display shows OK.
SXM | SXM connection | Check that the display shows OK. (Models with SXM only)
CAN | CAN connection | Check that the display shows OK.
Leather AMP | HK amplifier connection | Check with the {Audio Check} item. (Leather seat type with woofer)
Cloth AMP | HK amplifier connection | Check with the {Audio Check} item. (Cloth seat type with woofer)

2. CHECK VEHICLE SIGNALS WITH LINE DIAG MODE
1.

Turn the ignition switch to ACC.

2.

Press the button (b) twice with the button (a) pressed.

Pressing the button (a) for 3 seconds or more, or turning the ignition switch from the OFF to ACC position can exit the diagnostic mode.

3.

{Line Diag} screen is displayed.

4.

Check the signal status with the {Vehicle Signal} in the {Line Diag} screen.

Item | Contents | Inspection
Batt Volt | Battery voltage | Check that the battery voltage is displayed.
IG | IGN signal | Check that the display shows ON.
PKB | Parking brake signal | Pull the parking brake switch, and check that the display shows ON.
REV | Reverse signal | Place the select lever in reverse, and check that the display shows ON.
Bright | Bright signal | Turn the bright switch to ON, and check that the display shows ON.
SPEED | Speed pulse signal | Input the vehicle speed and check that it turns ON.
ILL+ | Illumination signal | Turn the lighting switch to ON, and check that the display shows OK.
Steering | Steering angle | Check that the steering operation is reflected on the display.

3. CHECK SPEAKER OUTPUT WITH LINE DIAG MODE AND ANTENNA CONNECTION
1.

Turn the ignition switch to ACC.

2.

Press the button (b) twice with the button (a) pressed.

Pressing the button (a) for 3 seconds or more, or turning the ignition switch from the OFF to ACC position can exit the diagnostic mode.

3.

{Line Diag} screen is displayed.

4.

Perform the speaker output check and antenna connection check with the {Audio Check} in the {Line Diag} screen.

Item | Contents | Inspection
MODE | Radio band switching | Check that the radio band (AM/FM) can be switched.
Seek UP/DOWN | Seek UP/DOWN operation | Check that the Seek UP/DOWN operation allows radio reception.
Speaker Check | Speaker check operation | Standard 4 speakers: Front right → front left → rear left → rear right speakers will sound in this order for 0.5 seconds each. 6 speakers: Front right → tweeter right → tweeter left → front left → rear left → rear right speakers will sound in this order for 0.5 seconds each. Brand: Tweeter left → front left → rear left → sub woofer → sub woofer → rear right → front right → tweeter right speakers will sound in order for 0.5 seconds each.

- The sound volume during the speaker check is different depending on the speakers.

  - Standard speaker: Sounds at 30 steps.

  - Brand speaker: Sounds at 25 steps.

- Turn the VOLUME button to control the sound volume.

4. CHECK MICROPHONE WITH LINE DIAG MODE
1.

Turn the ignition switch to ACC.

2.

Press the button (b) twice with the button (a) pressed.

Pressing the button (a) for 3 seconds or more, or turning the ignition switch from the OFF to ACC position can exit the diagnostic mode.

3.

{Line Diag} screen is displayed.

4.

Check the microphone level with the {Microphone} in the {Line Diag} screen.

Check that the microphone input level varies depending on the sound and voice.

ENTERTAINMENT & MONITORING > Audio System
NOTE

For procedure of each component in the audio system, refer to the respective sections.

- Audio unit: ENTERTAINMENT & MONITORING>Audio

- Power amplifier: ENTERTAINMENT & MONITORING>Power Amplifier

- Front speaker: ENTERTAINMENT & MONITORING>Front Speaker

- Rear speaker: ENTERTAINMENT & MONITORING>Rear Speaker

- Woofer: ENTERTAINMENT & MONITORING>Woofer

- Antenna: ENTERTAINMENT & MONITORING>Antenna

- Satellite switch assembly: ENTERTAINMENT & MONITORING>Switches and Harness

- External connection terminal: ENTERTAINMENT & MONITORING>External Connection Terminal

ENTERTAINMENT & MONITORING > Audio
REMOVAL
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>REMOVAL > CENTER GRILLE

3.

Remove the panel center UPR.

(1)

Release the clips and claws, then detach the panel center UPR.

4.

Remove the audio assembly.

(1)

Remove the screws.

(2)

Release the clips and disconnect the connector, and then remove the audio assembly.

5.

Remove the data communication module. (Model with telematics) ENTERTAINMENT & MONITORING>Data Communication Module>REMOVAL > DATA COMMUNICATION MODULE

6.

Remove the audio bracket.

(1)

Remove the screws, and then remove the audio bracket.

Remove the screws on RH side in the same procedure as on the LH side.

ENTERTAINMENT & MONITORING > Audio
INSTALLATION

Do not allow harness and cables to interfere with or get caught by other parts.

1.

Install the audio bracket.

2.

Install the data communication module. (Model with telematics) ENTERTAINMENT & MONITORING>Data Communication Module>INSTALLATION > DATA COMMUNICATION MODULE

3.

Install the audio assembly.

4.

Install the panel center UPR.

5.

Install the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>INSTALLATION > CENTER GRILLE

6.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Front Speaker
REMOVAL
1. TWEETER
1.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the trim panel assembly A pillar. EXTERIOR/INTERIOR TRIM>Upper Inner Trim>REMOVAL

3.

Remove the grille speaker side.

(1)

Release the clips, hooks and claws, then detach the grille speaker side.

4.

Remove the speaker assembly tweeter.

(1)

Remove the screws.

Preparation tool:

Stubby screwdriver

(2)

Disconnect the connector and remove the speaker assembly tweeter.

2. DOOR
1.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the trim panel front door. EXTERIOR/INTERIOR TRIM>Door Trim>REMOVAL > FRONT DOOR

3.

Remove the speaker assembly front.

(1)

Disconnect the connector.

(2)

Remove the screws and remove the speaker assembly front.

ENTERTAINMENT & MONITORING > Front Speaker
INSTALLATION
1. TWEETER
1.

Install the speaker assembly tweeter.

2.

Install the grille speaker side.

3.

Install the trim panel assembly A pillar. EXTERIOR/INTERIOR TRIM>Upper Inner Trim>INSTALLATION

4.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2. DOOR
1.

Install the speaker assembly front.

2.

Install the trim panel front door. EXTERIOR/INTERIOR TRIM>Door Trim>INSTALLATION

3.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Rear Speaker
REMOVAL
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the trim panel rear door. EXTERIOR/INTERIOR TRIM>Door Trim>REMOVAL > REAR DOOR

3.

Remove the speaker assembly rear.

(1)

Disconnect the connector.

(2)

Remove the screws and remove the speaker assembly rear.

ENTERTAINMENT & MONITORING > Rear Speaker
INSTALLATION
1.

Install the speaker assembly rear.

2.

Install the trim panel rear door. EXTERIOR/INTERIOR TRIM>Door Trim>INSTALLATION

3.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Woofer
REMOVAL
1.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the rear seat cushion assembly. SEATS>Rear Seat>REMOVAL

3.

Remove the trim panel assembly apron RH. EXTERIOR/INTERIOR TRIM>Rear Quarter Trim>REMOVAL

4.

Remove the speaker assembly woofer.

(1)

Disconnect the connector.

(2)

Remove the bolts and hooks, and then remove the speaker assembly woofer.

ENTERTAINMENT & MONITORING > Woofer
INSTALLATION
1.

Install the speaker assembly woofer.

Tightening torque:

7.5 N·m (0.8 kgf-m, 5.5 ft-lb)

2.

Install the trim panel assembly apron RH. EXTERIOR/INTERIOR TRIM>Rear Quarter Trim>INSTALLATION

3.

Install the rear seat cushion assembly. SEATS>Rear Seat>INSTALLATION

4.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Power Amplifier
REMOVAL

Remove the power amplifier assembly after sliding the front seat RH back and forth as necessary.

1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the power amplifier assembly.

(1)

Remove the harness clip, and disconnect each connector.

(2)

Remove the nut and remove the power amplifier assembly.

ENTERTAINMENT & MONITORING > Power Amplifier
INSTALLATION
1.

Install the power amplifier assembly.

Tightening torque:

7.5 N·m (0.8 kgf-m, 5.5 ft-lb)

2.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Antenna
REMOVAL
1. ROOF ANTENNA
1.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

2.

Lower the trim panel sub assembly. EXTERIOR/INTERIOR TRIM>Roof Trim>REMOVAL

Procedures for the trim panel sub assembly is performed inside the vehicle.

3.

Remove the antenna assembly roof.

(1)

Disconnect the connector and remove the nut.

For models with SXM, disconnect the SXM connector.

(2)

Remove the antenna assembly roof while pressing the temporal holding claws.

2. ANTENNA FEEDER CORD
•
INSTRUMENT PANEL
1.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>REMOVAL > CENTER GRILLE

3.

Remove the audio assembly or navigation assembly. ENTERTAINMENT & MONITORING>Audio>REMOVAL

4.

Remove the pocket assembly and the panel instrument passenger. EXTERIOR/INTERIOR TRIM>Glove Box>REMOVAL

5.

Remove the trim panel assembly A pillar RH. EXTERIOR/INTERIOR TRIM>Upper Inner Trim>REMOVAL

6.

Remove the cord assembly antenna feeder.

(1)

Disconnect the connector.

(2)

Release the harness clip and the clamp, and remove the cord assembly antenna feeder.

•
ROOF TRIM
7.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

8.

Remove the trim panel sub assembly. EXTERIOR/INTERIOR TRIM>Roof Trim>REMOVAL

9.

Remove the cord assembly antenna feeder.

3. TELEMATICS SUB ANTENNA
1.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>REMOVAL > CENTER GRILLE

3.

Remove the audio assembly or navigation assembly. ENTERTAINMENT & MONITORING>Audio>REMOVAL

4.

Remove the cover LWR driver. EXTERIOR/INTERIOR TRIM>Instrument Panel Lower Cover>REMOVAL

5.

Remove the combination meter assembly. INSTRUMENTATION/DRIVER INFO>Combination Meter>REMOVAL

6.

Remove the telematics sub antenna.

(1)

Disconnect the GPS antenna assembly connector.

(2)

Attach a string to the telematics sub antenna connector and the GPS antenna assembly connector on the main body side.

- A string makes operation easier during installation.

- The telematics sub antenna is integrated into the GPS antenna assembly cord.

(3)

Remove the bolts, cord clips and clamps, and pull out the telematics sub antenna from the combination meter side.

(4)

After the telematics sub antenna has been pulled out, remove the string attached to the connector in step (2).

Leave the attached string inside the instrument panel, and use it during installation.

4. GPS ANTENNA
1.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>REMOVAL > CENTER GRILLE

3.

Remove the audio assembly or navigation assembly. ENTERTAINMENT & MONITORING>Audio>REMOVAL

4.

Remove the cover LWR driver. EXTERIOR/INTERIOR TRIM>Instrument Panel Lower Cover>REMOVAL

5.

Remove the combination meter assembly. INSTRUMENTATION/DRIVER INFO>Combination Meter>REMOVAL

6.

Remove the GPS antenna assembly.

(1)

Disconnect the connector, and remove the connector clip.

(2)

Remove screws and remove the GPS antenna assembly.

(3)

Tie a string to the GPS antenna assembly connector on the vehicle side.

A string makes operation easier during installation.

(4)

Release the cord clamp, and pull out the GPS antenna assembly cord from the combination meter side.

(5)

When the GPS antenna assembly cord is pulled out, remove the string attached to the connector in step (3).

Leave the attached string inside the instrument panel, and use it during installation.

ENTERTAINMENT & MONITORING > Antenna
INSTALLATION
1. ROOF ANTENNA
1.

Install the antenna assembly roof.

Tightening torque:

4.5 N·m (0.5 kgf-m, 3.3 ft-lb)

2.

Install the trim panel sub assembly. EXTERIOR/INTERIOR TRIM>Roof Trim>INSTALLATION

3.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2. ANTENNA FEEDER CORD
•
INSTRUMENT PANEL
1.

Install the cord assembly antenna feeder.

2.

Install the trim panel assembly A pillar RH. EXTERIOR/INTERIOR TRIM>Upper Inner Trim>INSTALLATION

3.

Install the pocket assembly and the panel instrument passenger. EXTERIOR/INTERIOR TRIM>Glove Box>INSTALLATION

4.

Install the audio assembly or navigation assembly. ENTERTAINMENT & MONITORING>Audio>INSTALLATION

5.

Install the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>INSTALLATION > CENTER GRILLE

6.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

•
ROOF TRIM
1.

Install the cord assembly antenna feeder and the trim panel sub assembly. EXTERIOR/INTERIOR TRIM>Roof Trim>INSTALLATION

2.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

3. TELEMATICS SUB ANTENNA
1.

Install the telematics sub antenna.

Tightening torque:

7.5 N·m (0.8 kgf-m, 5.5 ft-lb)

Install the telematics sub antenna by using the sting left inside the parts to pull the part into the instrument panel.

2.

Install the combination meter assembly. INSTRUMENTATION/DRIVER INFO>Combination Meter>INSTALLATION

3.

Install the cover LWR driver. EXTERIOR/INTERIOR TRIM>Instrument Panel Lower Cover>INSTALLATION

4.

Install the audio assembly or navigation assembly. ENTERTAINMENT & MONITORING>Audio>INSTALLATION

5.

Install the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>INSTALLATION > CENTER GRILLE

6.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

4. GPS ANTENNA
1.

Install the GPS antenna assembly and GPS antenna assembly cord.

Install the GPS antenna assembly cord by using the sting left inside the parts to pull the part into the instrument panel.

2.

Install the combination meter assembly. INSTRUMENTATION/DRIVER INFO>Combination Meter>INSTALLATION

3.

Install the cover LWR driver. EXTERIOR/INTERIOR TRIM>Instrument Panel Lower Cover>INSTALLATION

4.

Install the audio assembly or navigation assembly. ENTERTAINMENT & MONITORING>Audio>INSTALLATION

5.

Install the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>INSTALLATION > CENTER GRILLE

6.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Switches and Harness
REMOVAL
1. SATELLITE SWITCH ASSEMBLY

Before handling the airbag system components, refer to “CAUTION” of “General Description” in “AIRBAG SYSTEM”. AIRBAG SYSTEM>General Description>CAUTION

1.

Set the tire to the straight-ahead position.

2.

Disconnect the ground terminal from the battery sensor, and wait for at least 60 seconds before starting work. REPAIR CONTENTS>NOTE > BATTERY

3.

Remove the driver’s airbag module. AIRBAG SYSTEM>Driver’s Airbag Module>REMOVAL

4.

Remove the steering wheel. POWER ASSISTED SYSTEM (POWER STEERING)>Steering Wheel>REMOVAL

5.

Remove the satellite switch assembly. POWER ASSISTED SYSTEM (POWER STEERING)>Steering Wheel>DISASSEMBLY

2. TELEMATICS BUTTON
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the light assembly map. LIGHTING SYSTEM>Spot Map Light>NOTE

3.

Remove the telematics button.

(1)

Remove the screws and remove the telematics button.

ENTERTAINMENT & MONITORING > Switches and Harness
INSTALLATION
1. SATELLITE SWITCH ASSEMBLY

- Before handling the airbag system components, refer to “CAUTION” of “General Description” in “AIRBAG SYSTEM”. AIRBAG SYSTEM>General Description>CAUTION

- Do not allow harness and connectors to interfere or get tangled up with other parts.

- If the steering wheel has been removed, make sure that the steering roll connector is not turned from the original position.

- If the steering wheel and steering angle sensor (steering roll connector) are removed, perform “VSC(VDC) Centering Mode” of the VDC. VEHICLE DYNAMICS CONTROL (VDC)>VDC Control Module and Hydraulic Control Unit (VDCCM&H/U)>ADJUSTMENT > VDC SENSOR MIDPOINT SETTING MODE

- Securely install the switch. Improper insertion of the pin or claw of the switch may cause improper installation.

1.

Install the satellite switch assembly. POWER ASSISTED SYSTEM (POWER STEERING)>Steering Wheel>ASSEMBLY

2.

Align the center position of the steering roll connector. AIRBAG SYSTEM>Roll Connector>ADJUSTMENT

3.

Install the steering wheel. POWER ASSISTED SYSTEM (POWER STEERING)>Steering Wheel>INSTALLATION

4.

Install the driver’s airbag module. AIRBAG SYSTEM>Driver’s Airbag Module>INSTALLATION

5.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2. TELEMATICS BUTTON
1.

Install the telematics button.

2.

Install the light assembly map. LIGHTING SYSTEM>Spot Map Light>NOTE

3.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Switches and Harness
INSPECTION
1. SATELLITE SWITCH ASSY
1.

Measure the resistance between connector terminals.

Preparation tool:

Circuit tester

Terminal No. | Inspection conditions | Standard
6 — 2 | SEEK (›) SEEK (‹) VOL (+) VOL (−) | A circuit is all OFF. | Approx. 100 kΩ
SEEK (›) | ON | Less than 1 Ω
SEEK (‹) | ON | Approx. 330 Ω
VOL (+) | ON | Approx. 1,000 Ω
VOL (−) | ON | Approx. 3,110 Ω
12 — 2 | SOURCE OFF HOOK/VOICE ON HOOK | B circuit is all OFF. | Approx. 100 kΩ
SOURCE | ON | Less than 1 Ω
OFF HOOK/VOICE | ON | Approx. 330 Ω
ON HOOK | ON | Approx. 1,000 Ω

2.

Apply battery voltage between the connector terminals to check lighting condition of illumination inside the switch.

When applying battery voltage, do not mix up the positive (+) side and the negative (−) side.

Incorrect polarity connection may cause LED damage inside the switch.

Terminal No. | Inspection conditions | Specification
10 (+) — 11 (−) | Apply battery voltage. | Light ON

3.

If it is found to be defective as a result of the measurement, replace the satellite switch assembly.

2. TELEMATICS BUTTON
1.

Check the button.

(1)

Measure the resistance between connector terminals.

Preparation tool:

Circuit tester

- SOS button

  Terminal No. | Inspection conditions | Standard
  6 — 1 | OFF | Approx. 1.6 kΩ
  ON | Less than 1 Ω

- i-button

  Terminal No. | Inspection conditions | Standard
  3 — 1 | OFF | Approx. 1.6 kΩ
  ON | Less than 1 Ω

(2)

Apply battery voltage between the connector terminals to check lighting condition of illumination inside the switch.

When applying battery voltage, do not mix up the positive (+) side and the negative (−) side.

Incorrect polarity connection may cause LED damage inside the switch.

Terminal No. | Inspection conditions | Specification
8 (+) — 2 (−) | Apply battery voltage. | Light ON

2.

Check the indicator.

(1)

Apply battery voltage between the connector terminals to check the lighting condition of the indicator.

When applying battery voltage, do not mix up the positive (+) side and the negative (−) side.

Incorrect polarity connection may cause LED damage inside the switch.

Terminal No. | Inspection conditions | Specification
4 (+) — 1 (−) | Apply battery voltage. | Illuminating in green
7 (+) — 1 (−) | Illuminating in red
4 (+) — 1 (−) and 8 (+) — 2 (−) | Apply battery voltage simultaneously. | Indicator turns on in dimmed condition at one level.
7 (+) — 1 (−) and 8 (+) — 2 (−) |

3.

Replace the telematics button if it is found defective.

ENTERTAINMENT & MONITORING > Microphone
NOTE

The microphone is integrated in the spot map light or stereo camera cover assembly.

For operation procedures, refer to “LIGHTING SYSTEM” section. LIGHTING SYSTEM>Spot Map Light

ENTERTAINMENT & MONITORING > Navigation System
WIRING DIAGRAM

Refer to “Audio and Navigation System” in the wiring diagram. WIRING SYSTEM>Audio and Navigation System>WIRING DIAGRAM

ENTERTAINMENT & MONITORING > Navigation System
INSPECTION

For inspection, refer to “Audio System”. ENTERTAINMENT & MONITORING>Audio System>INSPECTION

ENTERTAINMENT & MONITORING > Navigation System
OPERATION

For operation, refer to “Audio System”. ENTERTAINMENT & MONITORING>Audio System>OPERATION

ENTERTAINMENT & MONITORING > Navigation System
NOTE

For procedure of each component in the navigation system, refer to the respective section.

- Navigation unit: ENTERTAINMENT & MONITORING>Navigation Body

- GPS antenna: ENTERTAINMENT & MONITORING>Antenna

ENTERTAINMENT & MONITORING > Navigation Body
NOTE

For the operation procedures for navigation assembly, refer to “Audio”. ENTERTAINMENT & MONITORING>Audio

ENTERTAINMENT & MONITORING > Telematics System
WIRING DIAGRAM

Refer to “Telematics System” in the wiring diagram. WIRING SYSTEM>Telematics System>WIRING DIAGRAM

ENTERTAINMENT & MONITORING > Telematics System
INSPECTION
1. BASIC INSPECTION

For basic inspection, refer to “Basic Diagnostic Procedure” in “TELEMATICS SYSTEM (DIAGNOSTICS)”. TELEMATICS SYSTEM (DIAGNOSTICS)>Basic Diagnostic Procedure

2. SYSTEM BLOCK DIAGRAM

For system block diagram, refer to “System Block Diagram” in “TELEMATICS SYSTEM (DIAGNOSTICS)”. TELEMATICS SYSTEM (DIAGNOSTICS)>General Description>SYSTEM BLOCK DIAGRAM

3. MODULE I/O SIGNAL

For the specification (electrical component), refer to “Control Module I/O Signal” in “TELEMATICS SYSTEM (DIAGNOSTICS)”. TELEMATICS SYSTEM (DIAGNOSTICS)>Control Module I/O Signal>SPECIFICATION

ENTERTAINMENT & MONITORING > Telematics System
OPERATION
1. REGISTRATION (COMM CHECK)

Do not press and hold the i-button for more than two seconds during communication check, or settings will return to factory mode in poor radio wave environment. If the settings has returned to factory mode, perform the communication check again. To check the mode status, see “Subscription Status” in the current data display on Subaru Select Monitor.

1.

Replace the data communication module with a new part.

2.

Check that the LED of overhead console or stereo camera cover assembly illuminates in green.

3.

Register the immobilizer. For detailed operation procedure, refer to “Type B” or “Type D” described in “REGISTRATION MANUAL FOR IMMOBILIZER”.

4.

Press and hold the i-button for 2 seconds or more.

When the subscription is completed, the telematics system will automatically activate.

ENTERTAINMENT & MONITORING > Telematics System
NOTE

For procedure of each component in the telematics system, refer to the respective section.

- Data communication module: ENTERTAINMENT & MONITORING>Data Communication Module

- Antenna: ENTERTAINMENT & MONITORING>Antenna

- Telematics button: ENTERTAINMENT & MONITORING>Switches and Harness

ENTERTAINMENT & MONITORING > Data Communication Module
REMOVAL
1. DATA COMMUNICATION MODULE
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>REMOVAL > CENTER GRILLE

3.

Remove the audio assembly or navigation assembly. ENTERTAINMENT & MONITORING>Audio>REMOVAL

4.

Remove the data communication module.

(1)

Disconnect the cable connected to the audio assembly or navigation assembly.

(2)

Remove the screws and remove the data communication module.

Do not drop or apply any impact to the data communication module.

Remove the screws on LH side in the same procedure as on the RH side.

2. BACKUP BATTERY
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the data communication module. ENTERTAINMENT & MONITORING>Data Communication Module>REMOVAL > DATA COMMUNICATION MODULE

3.

Remove the backup battery.

(1)

Remove the screws, and then remove the battery cover.

Preparation tool:

TORX® T10

(2)

Disconnect the connector and remove the backup battery.

ENTERTAINMENT & MONITORING > Data Communication Module
INSTALLATION
1. DATA COMMUNICATION MODULE
1.

Install the data communication module.

Align the positioning pin (a) of the data communication module with the positioning hole of the audio assembly or navigation assembly.

2.

Install the audio assembly or navigation assembly. ENTERTAINMENT & MONITORING>Audio>INSTALLATION

3.

Install the grille ventilation assembly center. AIR CONDITIONER>Air Vent Grille>REMOVAL > CENTER GRILLE

4.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

5.

Perform the registration procedure and Bluetooth connection procedure if the data communication module is replaced with a new part.

- Registration procedure: ENTERTAINMENT & MONITORING>Telematics System>OPERATION

- Bluetooth connection procedure (audio without navigation): REPAIR CONTENTS>NOTE > Bluetooth CONNECTION PROCEDURE BETWEEN HEAD UNIT (AUDIO WITHOUT NAVIGATION) AND SMARTPHONE

6.

Check the LED illumination status of the telematics button. TELEMATICS SYSTEM (DIAGNOSTICS)>Check List for Interview>CHECK > LED ILLUMINATION STATUS LIST

2. BACKUP BATTERY
1.

Install the backup battery.

2.

Install the battery cover.

Tightening torque:

0.3 N·m (0.03 kgf-m, 0.2 ft-lb)

3.

Install the data communication module. ENTERTAINMENT & MONITORING>Data Communication Module>INSTALLATION > DATA COMMUNICATION MODULE

4.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Data Communication Module
INSPECTION
1. BACKUP BATTERY
1.

Measure the voltage between connector terminals.

Preparation tool:

Circuit tester

Terminal No. | Standard
1 (+) — 2 (−) | 2 V or more

2.

Replace the backup battery if the inspection result is not within the standard value.

ENTERTAINMENT & MONITORING > Camera
WIRING DIAGRAM

Refer to “Rearview Camera System” in the wiring diagram. WIRING SYSTEM>Rearview Camera System>WIRING DIAGRAM

ENTERTAINMENT & MONITORING > Camera
REMOVAL
1. REAR
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the trim panel assembly rear gate. EXTERIOR/INTERIOR TRIM>Rear Gate Trim>REMOVAL

3.

Remove the garnish assembly rear gate. EXTERIOR/INTERIOR TRIM>Rear Gate Garnish>REMOVAL

4.

Remove the rearview camera assembly.

Do not drop or apply any impact to the rearview camera because it is a precision equipment.

(1)

Disconnect the connector.

(2)

Disconnect the claws and then remove the rearview camera assembly.

ENTERTAINMENT & MONITORING > Camera
INSTALLATION
1. REAR
1.

Install the rearview camera assembly.

Press-in the rearview camera assembly until a locking sound is heard.

2.

Install the garnish assembly rear gate. EXTERIOR/INTERIOR TRIM>Rear Gate Garnish>INSTALLATION

3.

Install the trim panel assembly rear gate. EXTERIOR/INTERIOR TRIM>Rear Gate Trim>INSTALLATION

4.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

5.

Confirm the marker position. ENTERTAINMENT & MONITORING>Camera>INSPECTION

ENTERTAINMENT & MONITORING > Camera
INSPECTION
1. REAR
1.

Park the vehicle at the level place where there are enough area at the rear of the vehicle.

2.

Attach the tape as the target point for standard at the floor rearward of the vehicle as shown in the figure below.

Standard tape width is about 30 — 50 mm (1.18 — 1.97 in) and brilliant color shall be used.

(A) | Vehicle body center line
(B) | Rear edge of bumper
(C) | Target point

3.

Confirm the following before checking the corresponding items.

(1)

Rearview camera image is not displayed. (Everything except for the camera screen is displayed properly.)

1. Check the reverse signal with the {Vehicle Signal} screen in the Line Diag mode. ENTERTAINMENT & MONITORING>Audio System>OPERATION > CHECK VEHICLE SIGNALS WITH LINE DIAG MODE

2. Check the rear view camera connection status with the {Connection} screen in the Line Diag mode. ENTERTAINMENT & MONITORING>Audio System>OPERATION > CHECK CONNECTIONS WITH LINE DIAG MODE

(2)

The guide line is not displayed, or the guide line position is not aligned.

The rearview camera or its installation location on the vehicle may be deformed. Check the rearview camera and its installation location on the vehicle, and repair or replace if necessary.

ENTERTAINMENT & MONITORING > Accessory Power Supply Socket
WIRING DIAGRAM

For wiring diagrams related to the accessory power supply socket system, refer to the following items.

- Front: WIRING SYSTEM>Front Accessory Power Supply Socket System>WIRING DIAGRAM

- Rear: WIRING SYSTEM>Rear Accessory Power Supply Socket System>WIRING DIAGRAM

ENTERTAINMENT & MONITORING > Accessory Power Supply Socket
REMOVAL
1. FRONT
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the heater control assembly. AIR CONDITIONER>Control Panel>REMOVAL

3.

Remove the cover assembly front and the console box assembly. EXTERIOR/INTERIOR TRIM>Console Box>REMOVAL

4.

Remove the tray center UPR. EXTERIOR/INTERIOR TRIM>Center Console>REMOVAL

5.

Remove the socket assembly.

(1)

While releasing the claw, press it in from the rear to remove the socket assembly.

2. REAR
•
CONSOLE
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the cover assembly front and the console box assembly. EXTERIOR/INTERIOR TRIM>Console Box>REMOVAL

3.

Remove the socket assembly.

(1)

While releasing the claw, press it in from the rear to remove the socket assembly.

•
LUGGAGE ROOM
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the trim panel assembly apron LH. EXTERIOR/INTERIOR TRIM>Rear Quarter Trim>REMOVAL

3.

Remove the socket assembly.

(1)

While releasing the claw, press it in from the rear to remove the socket assembly.

ENTERTAINMENT & MONITORING > Accessory Power Supply Socket
INSTALLATION
1. FRONT
1.

Install the socket assembly.

Align the groove of the cover center socket with the claw of the socket assembly.

2.

Install the tray center UPR. EXTERIOR/INTERIOR TRIM>Center Console>INSTALLATION

3.

Install the console box assembly and the cover assembly front. EXTERIOR/INTERIOR TRIM>Console Box>INSTALLATION

4.

Install the heater control assembly. AIR CONDITIONER>Control Panel>INSTALLATION

5.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2. REAR
•
CONSOLE
1.

Install the socket assembly.

Align the groove of the console box assembly with the claw of the socket assembly.

2.

Install the cover assembly front and the console box assembly. EXTERIOR/INTERIOR TRIM>Console Box>INSTALLATION

3.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

•
LUGGAGE ROOM
1.

Install the socket assembly.

Align the groove of the trim panel assembly apron with the claw of the socket assembly.

2.

Install the trim panel assembly apron LH. EXTERIOR/INTERIOR TRIM>Rear Quarter Trim>INSTALLATION

3.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > External Connection Terminal
REMOVAL
1. FRONT
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the heater control assembly. AIR CONDITIONER>Control Panel>REMOVAL

3.

Remove the cover assembly front and the console box assembly. EXTERIOR/INTERIOR TRIM>Console Box>REMOVAL

4.

Remove the tray center UPR. EXTERIOR/INTERIOR TRIM>Center Console>REMOVAL

5.

Remove the AUX unit assembly.

(1)

While pressing the claw, press it in from the rear to remove the AUX unit assembly.

2. REAR
1.

Disconnect the ground terminal from battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2.

Remove the AUX unit assembly. EXTERIOR/INTERIOR TRIM>Console Box>DISASSEMBLY

ENTERTAINMENT & MONITORING > External Connection Terminal
INSTALLATION
1. FRONT
1.

Install the AUX unit assembly.

2.

Install the tray center UPR. EXTERIOR/INTERIOR TRIM>Center Console>INSTALLATION

3.

Install the console box assembly and the cover assembly front. EXTERIOR/INTERIOR TRIM>Console Box>INSTALLATION

4.

Install the heater control assembly. AIR CONDITIONER>Control Panel>INSTALLATION

5.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

2. REAR
1.

Install the AUX unit assembly. EXTERIOR/INTERIOR TRIM>Console Box>ASSEMBLY

2.

Connect the ground terminal to battery sensor. REPAIR CONTENTS>NOTE > BATTERY

ENTERTAINMENT & MONITORING > Diagnostics with Phenomenon
INSPECTION

For the diagnostics with phenomenon, refer to the “INFOTAINMENT SYSTEM (DIAGNOSTICS)” section. INFOTAINMENT(DIAGNOSTICS) >Diagnostics with Phenomenon

ENTERTAINMENT & MONITORING > Service Diagnostics Mode
NOTE

For the service diagnostic mode, refer to the “INFOTAINMENT SYSTEM (DIAGNOSTICS)” section. INFOTAINMENT(DIAGNOSTICS) >Service Diagnostics Mode