EXTERIOR/INTERIOR TRIM > General Description
COMPONENT

- The alphabet mark beside the clips in the figure indicates the colors of the clips.

- The clips with the same shape may have different engaging forces depending on their colors. Always use the specified parts when installing.

- The alphabets of color codes are used in the wiring diagram.

Color code | Collar | Color code | Collar | Color code | Collar
B | Black | R | Red | Br | Brown
G | Green | V | Violet | Gr | Gray
L | Blue | W | White | Lg | Light green
Or | Orange | Y | Yellow | Sb | Light blue
P | Pink | Be | Beige |  |

1. FRONT UNDER COVER

(1) | Under cover front |  |  | Tightening torque: N·m (kgf-m, ft-lb)
|  |  |  | T: | 18 (1.8, 13.3)

2. MUD GUARD

(1) | Mud guard front RH | (4) | Plate air flap front LH | (7) | Mud guard rear LH
(2) | Plate air flap front RH | (5) | Mud guard rear RH | (8) | Plate air flap rear LH
(3) | Mud guard front LH | (6) | Plate air flap rear RH |  |

3. FLOOR UNDER PROTECTOR

(1) | Under cover rear RH | (3) | Under cover rear LH | Tightening torque: N·m (kgf-m, ft-lb)
(2) | Protector tank RH | (4) | Protector tank LH | T1: | 7.5 (0.8, 5.5)
|  |  |  | T2: | 18 (1.8, 13.3)

For detailed exploded view of the fuel tank protector, refer to “Fuel Tank” in “FUEL INJECTION” section.

4. FRONT BUMPER

(1) | Grille ASSY front LWR | (9) | Light ASSY fog LH (other than LED type) | (17) | Energy absorber foam front
(2) | Bumper face front | (10) | Light ASSY fog LH (LED type) | (18) | Bracket grille front
(3) | Cover hook front | (11) | Bracket active grille shutter Front | (19) | Beam COMPL front
(4) | Bumper guard front | (12) | Active grille shutter | (20) | Air guide LH
(5) | Cover fog front LH (Type A model) | (13) | Stay bumper LWR side LH
(6) | Cover fog front LH (Type B model) | (14) | Stay bumper LWR center LH | Tightening torque: N·m (kgf-m, ft-lb)
(7) | Cover fog front LH (Type C model) | (15) | Bracket side front LH | T1: | 7.5 (0.8, 5.5)
(8) | Cover bumper cap | (16) | Bracket corner front LH | T2: | 32 (3.3, 23.6)

5. FRONT HOOD GRILLE

(1) | Ornament front | (3) | Bracket grille UPR | Tightening torque: N·m (kgf-m, ft-lb)
(2) | Grille ASSY front UPR | (4) | Panel COMPL front hood | T: | 4.5 (0.5, 3.3)

6. REAR BUMPER

(1) | Bumper beam COMPL rear | (7) | Bumper face rear | Tightening torque: N·m (kgf-m, ft-lb)
(2) | Cover side LWR LH | (8) | Reflex reflector LH | T1: | 7.5 (0.8, 5.5)
(3) | Bracket side rear LH | (9) | Cover bumper rear | T2: | 70 (7.1, 51.6)
(4) | Bracket corner rear LH | (10) | Bumper guard rear |  |
(5) | Grille air ventilation LH | (11) | Cover hook rear |  |
(6) | Cover side LWR RH | (12) | Reflex reflector RH

7. COWL PANEL

- Wiper model without nozzle

  (1) | Cowl panel side RH | (4) | Cover joint | (7) | Hose windshield washer
  (2) | Cowl panel | (5) | Cover cowl panel | (8) | Protector cowl panel
  (3) | Cowl panel side LH | (6) | Nozzle windshield washer | (9) | Seal cowl panel

- Wiper model with nozzle

  (1) | Cowl panel side RH | (5) | Cover cowl panel | (9) | Protector cowl panel
  (2) | Cowl panel | (6) | Joint washer hose | (10) | Seal cowl panel
  (3) | Cowl panel side LH | (7) | Nozzle windshield washer
  (4) | Cover joint | (8) | Hose windshield washer |  |

8. ROOF MOLDING

(1) | Cap lid | (5) | Fastener | Tightening torque: N·m (kgf-m, ft-lb)
(2) | Molding roof RH | (6) | Self-locking nut | T: | 7.5 (0.8, 5.5)
(3) | Rivet | (7) | Molding roof LH
(4) | Carrier BRKT |  |  |  |

9. ROOF RAIL

- Type A

  (1) | Roof rail ASSY RH | (8) | Rivet | Tightening torque: N·m (kgf-m, ft-lb)
  (2) | Seal washer | (9) | Fastener | T: | 7.5 (0.8, 5.5)
  (3) | Protector front RH | (10) | Roof rail ASSY LH |  |
  (4) | Protector center RH | (11) | Protector front LH |  |
  (5) | Protector rear RH | (12) | Protector center LH |  |
  (6) | Self-locking nut | (13) | Protector rear LH |  |
  (7) | Molding roof RH | (14) | Molding roof LH |  |

- Type B

  (1) | Roof rail ASSY RH | (8) | Rivet | Tightening torque: N·m (kgf-m, ft-lb)
  (2) | Seal washer | (9) | Fastener | T: | 7.5 (0.8, 5.5)
  (3) | Protector front RH | (10) | Roof rail ASSY LH |  |
  (4) | Protector center RH | (11) | Protector front LH |  |
  (5) | Protector rear RH | (12) | Protector center LH |  |
  (6) | Self-locking nut | (13) | Protector rear LH |  |
  (7) | Molding roof RH | (14) | Molding roof LH |  |

10. SIDE GARNISH & SIDE SPOILER

(1) | Garnish ASSY fender LH | (4) | Garnish ASSY front door LH (Type B) | (7) | Garnish ASSY rear quarter
(2) | Garnish ASSY front door LH (Type A) | (5) | Garnish ASSY rear door LH (Type B) | (8) | Garnish ASSY side sill
(3) | Garnish ASSY rear door LH (Type A) | (6) | Garnish ASSY rear door UPR |  |

11. REAR GATE GARNISH

- Type A

  (1) | Garnish bracket side LH | (6) | Garnish ASSY rear gate | Tightening torque: N·m (kgf-m, ft-lb)
  (2) | Opener switch (model with lock/unlock button)/opener switch (model without lock/unlock button) | (7) | Camera cover | T: | 4.5 (0.5, 3.3)
  (3) | Bracket | (8) | Protector
  (4) | Garnish bracket side RH | (9) | Garnish ASSY rear gate LWR
  (5) | Protector UPR | (10) | Ornament rear

- Type B

  (1) | Garnish bracket side LH | (6) | Garnish ASSY rear gate | Tightening torque: N·m (kgf-m, ft-lb)
  (2) | Opener switch (model with lock/unlock button)/opener switch (model without lock/unlock button) | (7) | Camera cover | T: | 4.5 (0.5, 3.3)
  (3) | Bracket | (8) | Protector
  (4) | Garnish bracket side RH | (9) | Garnish ASSY rear gate LWR
  (5) | Protector UPR | (10) | Ornament rear

12. ROOF SPOILER

- Type A

  (1) | Spoiler ASSY roof CTR | (3) | Spoiler ASSY roof side RH | Tightening torque: N·m (kgf-m, ft-lb)
  (2) | Spoiler ASSY roof side LH | (4) | Stop light ASSY high-mounted | T1: | 4.5 (0.5, 3.3)
  |  |  |  | T2: | 7.5 (0.8, 5.5)

- Type B

  (1) | Spoiler ASSY roof CTR | (3) | Spoiler ASSY roof side RH | Tightening torque: N·m (kgf-m, ft-lb)
  (2) | Spoiler ASSY roof side LH | (4) | Stop light ASSY high-mounted | T1: | 4.5 (0.5, 3.3)
  |  |  |  | T2: | 7.5 (0.8, 5.5)

13. DOOR TRIM

(1) | Weather strip front door INN | (5) | Switch ASSY power window SUB front | (9) | Trim panel rear door
(2) | Trim panel front door | (6) | Switch ASSY power window MAIN front | (10) | Switch ASSY power window SUB rear
(3) | Light ASSY door step | (7) | Remote ASSY door | (11) | Weather strip rear door INN
(4) | Seat position memory switch ASSY | (8) | Cap remote | (12) | Cover gusset

14. CONSOLE BOX

(1) | Cover ASSY front | (13) | Cover rear seat heater RH | (25) | Cord ASSY power
(2) | Bracket console COMPL | (14) | Switch ASSY rear seat heater RH | (26) | Cord ASSY rear seat heater
(3) | Cap console RH | (15) | AUX unit rear | (27) | Duct console rear
(4) | Console box LWR RH | (16) | AUX cap | (28) | Tape (model with rear seat heater)
(5) | Switch cap | (17) | Lid ASSY console | (29) | Grille ASSY console rear
(6) | Switch ASSY hand brake | (18) | Tray ASSY console | (30) | Cover rear console ASSY
(7) | Tray | (19) | Mat console box | (31) | Pocket console rear
(8) | X mode switch | (20) | Cord ASSY console | (32) | Panel switch console
(9) | Switch ASSY front seat heater | (21) | Pocket console |
(10) | Cap (model without front seat heater) | (22) | Duct console center | Tightening torque: N·m (kgf-m, ft-lb)
(11) | Socket ASSY | (23) | Cup holder | T1: | 6.5 (0.7, 4.8)
(12) | Cup holder cover front | (24) | Mat cover front | T2: | 18 (1.8, 13.3)

15. INSTRUMENT PANEL

(1) | Grille speaker side LH | (10) | Switch ASSY instrument panel | (19) | Tray center UPR
(2) | Grille front defroster | (11) | Ornament panel ASSY driver | (20) | AUX unit front
(3) | Sunload sensor | (12) | Cover starter switch (model without push button ignition starter) | (21) | Socket ASSY
(4) | Grille speaker side RH | (13) | Panel starter switch (model with push button ignition starter) | (22) | Light pocket
(5) | Panel COMPL instrument | (14) | Switch ASSY starter (model with push button ignition starter) | (23) | Ornament panel console COMPL LH
(6) | Cover ASSY instrument panel side LH | (15) | Mat center tray | (24) | Cover center side LH
(7) | Cover ASSY instrument panel side RH | (16) | Tray center LWR | (25) | Cover center side RH
(8) | Cover LWR driver | (17) | Ornament ASSY passenger | (26) | Ornament panel console COMPL RH
(9) | Fuse box front lid | (18) | Duct console front

(1) | Grille defroster side LH | (5) | Combination meter ASSY | (9) | Switch ASSY meter
(2) | Panel COMPL instrument | (6) | Grille ventilation ASSY center LH | (10) | Visor ASSY
(3) | Grille defroster side RH | (7) | Grille ventilation ASSY center RH | (11) | Cover steering UPR
(4) | Grille ventilation side LH | (8) | Grille ventilation side RH |  |

(1) | Driver monitoring unit | (9) | Antenna ASSY telematics | (16) | Panel center UPR
(2) | Panel display UPR (model with driver monitoring unit) | (10) | GPS antenna ASSY | (17) | Heater control ASSY
(3) | Panel display LWR (model with driver monitoring unit) | (11) | Reinforcement meter | (18) | Panel ASSY heater
(4) | Panel display UPR (model without driver monitoring unit) | (12) | Bracket audio LH | (19) | Backup unit ASSY
(5) | Panel display LWR (model without driver monitoring unit) | (13) | Audio ASSY |  |
(6) | Multi-function display | (14) | Bracket audio RH | Tightening torque: N·m (kgf-m, ft-lb)
(7) | Panel COMPL instrument | (15) | Cover center UPR | T: | 7.5 (0.8, 5.5)
(8) | Keyless access CM |  |  |  |

(1) | Panel COMPL instrument | (5) | Pocket COMPL | (9) | Light pocket cover
(2) | Under cover ASSY passenger | (6) | Cushion pocket | (10) | Light pocket
(3) | Reinforcement passenger | (7) | Damper ASSY
(4) | Panel instrument passenger | (8) | Key cylinder ASSY

(1) | Beam steering COMPL | (7) | Reinforcement CTR LWR | Tightening torque: N·m (kgf-m, ft-lb)
(2) | TORX® bolt (M8 × 57) | (8) | Panel COMPL instrument | T1: | 7.5 (0.8, 5.5)
(3) | Cap bolt | (9) | TORX® bolt (M8 × 37) | T2: | 25 (2.5, 18.4)
(4) | Adjuster clip space | (10) | Passenger’s airbag module ASSY
(5) | Knee airbag module ASSY | (11) | Center bracket UPR
(6) | Cushion

(1) | Nozzle front defroster ASSY | (4) | Duct center ventilation front | (7) | Duct grille ventilation CTR RH
(2) | Duct side defroster LH | (5) | Duct grille ventilation CTR LH | (8) | Duct side ventilation RH
(3) | Duct side ventilation LH | (6) | Panel COMPL instrument | (9) | Duct side defroster RH

16. INNER TRIM

(1) | Tether clip | (8) | Cover catcher | (15) | Remote control back rest switch
(2) | Trim panel ASSY A pillar | (9) | Trim panel ASSY C pillar | (16) | Socket ASSY
(3) | Cover side sill front FT RH | (10) | Cover belt |
(4) | Cover side sill front RR RH | (11) | Trim panel ASSY rear pillar UPR | Tightening torque: N·m (kgf-m, ft-lb)
(5) | Trim panel ASSY B pillar LWR | (12) | Trim panel ASSY apron | T: | 7.5 (0.8, 5.5)
(6) | Trim panel ASSY B pillar UPR | (13) | Luggage hook
(7) | Cover side sill rear UPR | (14) | Cover lid |  |
∗: 6 pieces on the LH side For model without sub woofer, 6 pieces on the RH side; for model with sub woofer, 5 pieces on the RH side

(1) | Spacer rear floor front | (5) | Cover trunk | (9) | Mat rear floor side LH
(2) | Board rear floor front RH | (6) | Spacer rear floor side LH | (10) | Cover rear floor edge ASSY
(3) | Board rear floor front LH | (7) | Mat rear floor side RH |  |
(4) | Spacer rear floor side RH | (8) | Mat floor CTR |  |

17. REAR GATE TRIM

(1) | Trim panel ASSY rear gate side RH | (5) | Trim panel rear gate handle | (9) | Cap rear gate LH
(2) | Trim panel ASSY rear gate LWR | (6) | Light ASSY rear gate | (10) | Trim panel ASSY rear gate UPR
(3) | Cap rear gate RH | (7) | Cap rear gate LWR | (11) | Trim panel ASSY rear gate side LH
(4) | Luggage hook | (8) | Power rear gate inner switch ASSY

For the detailed exploded view for power rear gate inner switch assembly, refer to “Module & Rear Gate” in “POWER REAR GATE SYSTEM” section. POWER REAR GATE SYSTEM>General Description>COMPONENT

18. ROOF TRIM

(A) | Model with sunroof | (B) | Models without EyeSight | (C) | Model without sunroof
(1) | Trim panel sub ASSY (model with sunroof) | (3) | Holder cover ELR | (5) | Garnish sunroof
(2) | Holder | (4) | Cap belt roof | (6) | Trim panel sub ASSY (model without sunroof)

19. ROOM INNER PARTS

(1) | Sun visor ASSY RH | (4) | Mirror ASSY rearview inner | (6) | Hook sun visor
(2) | Cap sun visor | (5) | Sun visor ASSY LH | (7) | Assist grip
(3) | Base inner mirror |  |

For exploded view of the inner mirror, refer to “Rearview Mirror” in “GLASS/WINDOWS/MIRRORS” section. GLASS/WINDOWS/MIRRORS>General Description>COMPONENT > REAR VIEW MIRROR

20. FLOOR MAT

(1) | Insulator toe board | (4) | Foot pad (resin type) | Tightening torque: N·m (kgf-m, ft-lb)
(2) | Plate footrest | (5) | Insulator tunnel | T: | 7.5 (0.8, 5.5)
(3) | Floor mat | (6) | Accelerator plate