WIRING SYSTEM
WI

WIRING SYSTEM > How To Read Wiring Diagrams
NOTE

Refer to HELP on how to read the wiring diagram.

WIRING SYSTEM > List of Signal Name
LIST
1. A/C CONTROL PANEL

Abbr. | Full name
5V | 5V power supply
A/C CUT | A/C cut signal
ACC | ACC power supply
BATT | Battery power supply
CAN H | CAN HI
CAN L | CAN LO
COMP C/V | Variable compressor solenoid valve
EVA SSR | Post evaporator sensor
FAN CNT | Fan control signal
FAN ON | Blower fan ON signal
FRE → REC | Intake door actuator (recirc)
GND | GND
HAZARD | Hazard switch
HEAT COR SSR | Heater core sensor
IGN | Ignition power supply
ILL − | Illumination power supply (−)
ILL + | Illumination power supply (+)
INT POT | Intake door potentiometer signal
IN-VEH SSR | In-vehicle sensor
LEFT MIX #1 | Air mix door actuator LH #1
LEFT MIX #2 | Air mix door actuator LH #2
LEFT MIX #3 | Air mix door actuator LH #3
LEFT MIX #4 | Air mix door actuator LH #4
MIX #1 | Air mix door actuator #1
MIX #2 | Air mix door actuator #2
MIX #3 | Air mix door actuator #3
MIX #4 | Air mix door actuator #4
MODE #1 | Mode door actuator #1
MODE #2 | Mode door actuator #2
MODE #3 | Mode door actuator #3
MODE #4 | Mode door actuator #4
MOIST SSR | Humidity sensor
PD.S | Pressure sensor (discharge)
PH.S | Pressure sensor
REC → FRE | Intake door actuator drive signal (fresh)
RIGHT MIX #1 | Air mix door actuator RH #1
RIGHT MIX #2 | Air mix door actuator RH #2
RIGHT MIX #3 | Air mix door actuator RH #3
RIGHT MIX #4 | Air mix door actuator RH #4
SENSOR GND | GND for sensors
SH (L) GND | Seat heater (L) GND
SH (R) GND | Seat heater (R) GND
SH CONT (L) | Seat heater control (L)
SH CONT (R) | Seat heater control (R)
SH SENSOR (L) | Seat heater sensor (L)
SH SENSOR (R) | Seat heater sensor (R)
SUN SSR | Sunload sensor

2. AIRBAG CM

Abbr. | Full name
+B | Battery power
ACL | OBD connector
CANH | Can communication line H
CANL | Can communication line L
CSL− | Side sensor C-pillar LH (−)
CSL+ | Side sensor C-pillar LH (+)
CSR− | Side sensor C-pillar RH (−)
CSR+ | Side sensor C-pillar RH (+)
D1− | Driver-side airbag (1st stage) (−)
D1+ | Driver-side airbag (1st stage) (+)
D2− | Driver-side airbag (2nd stage) (−)
D2+ | Driver-side airbag (2nd stage) (+)
DK− | Driver-side knee airbag (−)
DK+ | Driver-side knee airbag (+)
DSL− | Side sensor front door LH (−)
DSL+ | Side sensor front door LH (+)
DSR− | Side sensor front door RH (−)
DSR+ | Side sensor front door RH (+)
FSL− | Occupant detection system (airbag control) (RHD) (−)
FSL+ | Occupant detection system (airbag control) (RHD) (+)
FSR− | Occupant detection system (airbag control) (−)
FSR+ | Occupant detection system (airbag control) (+)
GND | Ground
GW2 | DCM (emergency call)
GW3 | BIU (unlocked the door in the event of collision)
ICL− | Curtain airbag module LH (−)
ICL+ | Curtain airbag module LH (+)
ICR− | Curtain airbag module RH (−)
ICR+ | Curtain airbag module RH (+)
IGN | IG switch
LSP− | Seat position sensor LH (−)
LSP+ | Seat position sensor LH (+)
P1− | Passenger-side airbag (1st stage) (−)
P1+ | Passenger-side airbag (1st stage) (+)
P2− | Passenger-side airbag (2nd stage) (−)
P2+ | Passenger-side airbag (2nd stage) (+)
PAL1− | Pedestrian protection (airbag) (−)
PAL1+ | Pedestrian protection (airbag) (+)
PAV− | Passenger-side active vent (−)
PAV+ | Passenger-side active vent (+)
PFL− | Pretensioner front LH (−)
PFL+ | Pretensioner front LH (+)
PFL2− | Double-pretensioner LH (−)
PFL2+ | Double-pretensioner LH (+)
PFR− | Pretensioner front RH (−)
PFR+ | Pretensioner front RH (+)
PFR2− | Double-pretensioner RH (−)
PFR2+ | Double-pretensioner RH (+)
PLA− | Adaptive belt LH (−)
PLA+ | Adaptive belt LH (+)
PRA− | Adaptive belt RH (−)
PRA+ | Adaptive belt RH (+)
PRL− | Pretensioner rear LH (−)
PRL+ | Pretensioner rear LH (+)
PRR− | Pretensioner rear RH (−)
PRR+ | Pretensioner rear RH (+)
PSL− | Pedestrian protection sensor LH (−)
PSL+ | Pedestrian protection sensor LH (+)
PSR− | Pedestrian protection sensor RH (−)
PSR+ | Pedestrian protection sensor RH (+)
RSP− | Seat position sensor RH (−)
RSP+ | Seat position sensor RH (+)
SFL− | Side airbag module LH (−)
SFL+ | Side airbag module LH (+)
SFR− | Side airbag module RH (−)
SFR+ | Side airbag module RH (+)
SL− | Front sensor LH (−)
SL+ | Front sensor LH (+)
SR− | Front sensor RH (−)
SR+ | Front sensor RH (+)
SSL− | Side sensor B-pillar LH (−)
SSL+ | Side sensor B-pillar LH (+)
SSR− | Side sensor B-pillar RH (−)
SSR+ | Side sensor B-pillar RH (+)
SSS− | Side sensor safing (−)
SSS+ | Side sensor safing (+)
TSNS− | Temperature sensor for pedestrian protection (−)
TSNS+ | Temperature sensor for pedestrian protection (+)

3. AUDIO AMPLIFIER

Abbr. | Full name
+B | Backup power supply
+B2 | Backup power supply 2
ACC | ACC power supply
FL− | LH front door speaker (−)
FL+ | LH front door speaker (+)
FR− | RH front door speaker (−)
FR+ | RH front door speaker (+)
GND | GND
GND2 | GND 2
II1− | Interrupt voice input (−)
II1+ | Interrupt voice input (+)
L− | LH main voice input (−)
L+ | LH main voice input (+)
MUTE | Mute
R− | RH main voice input (−)
R+ | RH main voice input (+)
RL− | LH rear door speaker (−)
RL+ | LH rear door speaker (+)
RR− | RH rear door speaker (−)
RR+ | RH rear door speaker (+)
SLD | Shield GND
SLD2 | Shield GND 2
TWL− | LH side tweeter (−)
TWL+ | LH side tweeter (+)
TWR− | RH side tweeter (−)
TWR+ | RH side tweeter (+)
TX− | CAN communication (−)
TX+ | CAN communication (+)
WF1− | Woofer 1 (−)
WF1+ | Woofer 1 (+)
WF2− | Woofer 2 (−)
WF2+ | Woofer 2 (+)

4. AUDIO/NAVIGATION UNIT

Abbr. | Full name
+5V | 5V power supply
USB power supply
+ACC | ACC power supply
+B | Backup power supply
6V+ | 6 V power supply
AMP CAN− | Amplifier CAN (−)
AMP CAN+ | Amplifier CAN (+)
AMP MUTE | Amplifier mute signal
ANT-ON | Antenna power supply
BRIGHT | Bright signal
CA− | Camera input (−)
CA+ | Camera input (+)
CAN− | CAN communication (−)
CAN+ | CAN communication (+)
DAB SIGNAL | DAB signal
DCM MUTE | DCM mute signal
DET | Microphone detection
FL− | LH front door speaker (−)
FL+ | LH front door speaker (+)
FM/AM | FM/AM radio signal
FR− | RH front door speaker (−)
FR+ | RH front door speaker (+)
FRONT ON | Pin jack insertion detection
GND | GND
GPS | GPS signal
IGN | Ignition power supply
ILL− | Illumination (−)
ILL+ | Illumination (+)
INT− | Amplifier CAN (−)
INT+ | Amplifier CAN (+)
L SIG | LH AUX input
MIC− | Microphone input (−)
MIC+ | Microphone input (+)
MIC2− | Microphone input 2 (−)
MIC2+ | Microphone input 2 (+)
PKB | Parking brake signal
R SIG | RH AUX input
R/L SIG | AUX input shield GND
REVERSE | Reverse signal
RL− | LH rear door speaker (−)
RL+ | LH rear door speaker (+)
RR− | RH rear door speaker (−)
RR+ | RH rear door speaker (+)
SGND | Shield GND
SLD2 | Shield GND 2
SPEED | Speed signal
STEERING GND | Steering switch GND
STEERING SW 1+ | Steering switch 1 (+)
STEERING SW 2+ | Steering switch 2 (+)
USB− | USB signal (−)
Data signal (−)
USB+ | USB signal (+)
Data signal (+)
VCC | Microphone power supply
XM/DAB SIGNAL | Sirius XM signal

5. AUTO HEADLIGHT BEAM LEVELER CM

Abbr. | Full name
+B | Battery power supply
CAN-H | CAN-H
CAN-L | CAN-L
E1 | GND
IG | Ignition power supply
LAG | Leveling actuator GND
LAS | Leveling actuator signal
LAV | Leveling actuator power supply
L-DIAG | LH headlight malfunction signal
R-DIAG | RH headlight malfunction signal
SAG | SRH & ADB actuator GND
SAS | SRH & ADB actuator LIN signal
SRH−SW | SRH OFF switch

6. BODY INTEGRATED UNIT

Abbr. | Full name
ACC SW | ACC SW
AN GND | Spare analog input GND
ARM | ARM output
BAT (BU) | BAT (backup)
BAT (ILU) | BAT (illumination)
BAT (L HL_H) | BAT (headlight Hi LH) (LHB)
BAT (R HL_H) | BAT (headlight Hi RH) (RHB)
BAT (S LK/KEY LK/TURN) | BAT (shift lock/key lock/turn light)
BAT (SIG) | BAT (control system)
BAT (TL) | BAT (tail)
BUZZER | Answer-back buzzer output
C/P LED | Charge port LED output
C/P SW | Charge port SW
CAN_H (B) | Body CAN H
CAN_H (DIAG) | Diagnostic CAN H
CAN_H (M) | Main CAN H
CAN_L (B) | Body CAN L
CAN_L (DIAG) | Diagnostic CAN L
CAN_L (M) | Main CAN L
COL SIG | Collision detection signal
D KEY SW (L) | Door key SW (lock)
D KEY SW (UL) | Door key SW (unlock)
D LK (D_UL) | Door lock output (driver's seat unlock)
D LK (DLK/P_UL) | Door lock output (double lock or passenger's seat unlock)
D LK SW (D) | Door lock status SW (driver's seat)
D LK SW (P) | Door lock status SW (passenger's seat)
D O/C | Door open/close status output
D SW (D) | Door switch (driver's seat)
D SW (P) | Door SW (passenger's seat)
D SW (RG) | Door SW (rear gate/trunk)
D SW (RL) | Door SW (RL: rear left seat)
D SW (RR) | Door SW (RR: rear right seat)
DIM PASS SW | Dimmer pass SW
DIM_H SW | Dimmer Hi SW
DRL | DRL output
DSM | DISARM output
F FOG RLY | Front fog light relay output
F FOG SW | Front fog light SW
F WASH SW | Front washer switch
F WIP | Front wiper RTN
F WIP SW (AUTO) | Front wiper AUTO SW
F WIP_H RLY | Front wiper Hi relay output (redundant circuit)
F WIP_H RLY (SIG) | Front wiper Hi relay output (control side)
F WIP_H SW | Front wiper Hi SW (redundant circuit)
F WIP_H SW (SIG) | Front wiper Hi SW (control)
F WIP_L RLY (SIG) | Front wiper Lo relay output
F WIP_L SW | Front wiper Lo SW
F/L OP SW | Fuel lap opener SW
F/L ST SW | Fuel lap status SW
FL TURN | Turn light output LH front
FR TURN | Turn light output RH front
FUEL LID | Fuel unlock output
GND | GND
HAZ SW | Turn hazard SW
HOOD SW (C) | Hood SW input (close side)
HOOD SW (O) | Hood SW input (open side)
I/V LED L | Passenger room LED LH output
I/V LED R | Passenger room LED RH output
ILU | Illumination output
IMM | EGI - immobilizer communication
IMM (A) | Immobilizer antenna (A)
IMM (B) | Immobilizer antenna (B)
IMP SSR | Impact sensor
KEY ILU H | Key ring illumination output (light)
KEY ILU L | Key ring illumination output (LED)
KEY LK | Key lock solenoid output
KEY_IN | Key-in SW
L HL_H | Headlight Hi LH output (LHOUT)
L OFF SW | LANE OFF SW
LGT RLY | Lighting relay power supply (redundant circuit)
LGT RLY (SIG) | Lighting relay power supply (control side)
LGT SSR | Illumination sensor signal
LGT SSR +B | Power supply for illumination sensor
LGT SSR GND | Illumination sensor GND
LGT SW (AUTO) | Lighting switch AUTO
LGT SW1 | Lighting 1 SW
LGT SW2 | Lighting 2 SW (redundant circuit)
LGT SW2 (SIG) | Lighting 2 SW (control)
LGT_L RLY | Lighting Lo relay output (redundant circuit)
LGT_L RLY (SIG) | Lighting Lo relay output (control side)
LIN 1 | LIN 1
LIN 2 | LIN 2
LIN 3 | LIN 3
LUG | Luggage/trunk light output
M LK SW | Manual lock SW
M UL SW | Manual unlock SW
MAP | Map light output
OPN SW (RG) | Opener SW (rear gate)
P SW | P range SW
P/U | Spare pull up input
P-CR OFF SW | P-CR OFF SW
R DEF | Rear defogger output
R DEF SW | Rear defogger SW
R FOG RLY | Rear fog light relay output
R FOG SW | Rear fog light SW
R HL_H | Headlight Hi RH output (RHOUT)
R WASH SW | Rear washer SW
R WIP | Rear wiper RTN
R WIP RLY | Rear wiper relay output
R WIP SW | Rear wiper SW (ON)
R WIP SW (INT) | Rear wiper SW (INT)
RAIN GND | Sensitivity adjustment GND
RAIN SIG | Sensitivity adjustment SIG
RE SW | MT reverse SW
RL TURN | Turn light output LH rear
ROOM | Room light output
RR TURN | Turn light output RH rear
S D/M LGT | Side door mirror light output
S LK | Shift lock solenoid output
S/B SW | Parking brake SW
S/HO | Security horn output
SC SI | Security siren output
SCR IND | Security light output
SRF OFF | SRF OFF SW
SRF RLY L | SRF (L) relay output
SRF RLY R | SRF (R) relay output
STL SW | Stop light switch
T/L RLY | Tail light relay output
TL | Tail light output
TLR | Towing SW
TURN L SW | Turn signal LH SW
TURN R SW | Turn signal RH SW
WIP DCR | Wiper deicer output

7. COMBINATION METER

Abbr. | Full name
BATT | Battery power supply
BRIGHT SIGNAL | Bright signal
BRIGHT SW | Bright switch
CAN (−) | CAN (−)
CAN (+) | CAN (+)
CAR ACCESS ALARM OFF | Pedestrian alert OFF
FUEL SENDER | Fuel gauge
FUEL SENDER GND | Fuel gauge GND
GND | GND
IGN | Ignition power supply
ILLUMI (−) | Illumination (−)
ILLUMI CONTROL SW GND | Illumination control switch GND
ILLUMI CONTROL SW POWER | Illumination control switch
ILLUMI CONTROL SW VR | Illumination control switch VR
IMB/SECURITY | Immobilizer/security
ISS SW | Auto start stop cancel switch
LO | Dual-range LO
ODO/TRIP SW | ODO/TRIP switch
ODO/TRIP SW GND | ODO/TRIP switch GND
OIL | Engine oil
OUTSIDE TEMP | Ambient air temperature
OUTSIDE TEMP GND | Ambient air temperature GND
PEDESTRIAN OUTSIDE TEMP | Pedestrian temperature sensor
PEDESTRIAN OUTSIDE TEMP GND | Pedestrian temperature sensor GND
R.DIFFTEMP | Rear differential oil temperature
R.DIFFTEMP GND | Rear differential oil temperature GND
REARSEATBELT (C) | Rear seat belt center
REARSEATBELT (L) | Rear seat belt LH
REARSEATBELT (R) | Rear seat belt RH
SEATBELT (D) | Driver's seat belt
SEATBELT (P) | Passenger's seat belt
SI-DRIVE (+) | SI-DRIVE (+)
TFT SW | Steering switch
TURN (L) | Turn signal light LH
TURN (R) | Turn signal light RH
U-ART1 | U-ART 1
U-ART2 | U-ART 2
U-ART3 | U-ART 3
WASHER | Washer
X-MODE SW | X mode switch

8. DATA COMMUNICATION MODULE

Abbr. | Full name
ACC | ACC power supply
AIRBAG | Auto collision notice
BCAN _H | High-body CAN
BCAN_L | Low-body CAN
BUTTON_RS | I call switch input
BUTTON_SOS | SOS switch input
FT_LH− IN | LH speaker input (−)
FT_LH− OUT | LH speaker output (−)
FT_LH+ IN | LH speaker input (+)
FT_LH+ OUT | LH speaker output (+)
FT_RH− IN | RH speaker input (−)
FT_RH− OUT | RH speaker output (−)
FT_RH+ IN | RH speaker input (+)
FT_RH+ OUT | RH speaker output (+)
GND | GND
GPS RF | GNSS signal
IGN | Ignition power supply
LED_GREEN | Switch indicator (green)
LED_RED | Switch indicator (red)
MCAN_H | High-main CAN
MCAN_L | Low-main CAN
MIC GND IN | Microphone input (−)
MIC GND OUT | Microphone output (−)
MIC S GND | Shield GND
MIC SIGNAL IN | Microphone input (+)
MIC SIGNAL OUT | Microphone output (+)
MIC_5V | Microphone power supply
MUTE | Mute
PRIMARY LTE RF | TEL antenna signal main
SECONDARY LTE RF | TEL antenna signal sub
USB_D− | Data signal (−)
USB_D+ | Data signal (+)
USB_VBUS | USB power supply
VBATT | Battery power supply

9. DC/DC CONVERTER 1

Abbr. | Full name
GND | GND
INPUT (ACC) | Input (ACC)
INPUT (B1) | Input (battery 1)
INPUT (B2) | Input (battery 2)
INPUT (IGN) | Input (ignition)
INPUT (ISS) | Input (auto start stop)
LIN | LIN
OUTPUT (ACC) | Output (ACC)
OUTPUT (B1) | Output (battery 1)
OUTPUT (B2) | Output (battery 2)
OUTPUT (IGN) | Output (ignition)

10. DC/DC CONVERTER 2

Abbr. | Full name
GND | GND
INPUT (+B1) | Input (battery 1)
INPUT (+B2) | Input (battery 2)
INPUT (IGN) | Input (ignition)
INPUT (ISS) | Input (auto start stop)
LIN | LIN
OUTPUT (+B1) | Output (battery 1)
OUTPUT (+B2) | Output (battery 2)

11. DRIVER MONITORING UNIT

Abbr. | Full name
+B | Battery power supply
CANH | High-speed CAN High
CANL | High-speed CAN Low
GND | GND
OFF SW | Driver monitoring system OFF switch

12. ECM

Abbr. | Full name
ACCM | Accelerator sensor (main)
ACCR | ACC cut
ACCS | Accelerator sensor (sub)
ACP | Air conditioner middle pressure SW
ACRLY | Air conditioner relay
ACSW | Air conditioner SW
AFM | Air flow sensor
AFR− | A/F sensor (−)
AFR+ | A/F sensor (+)
AFSLD | Shield (A/F sensor)
ANGS | MCV angle sensor
AVCC1 | VCC 1 (engine)
AVCC2 | VCC (air flow sensor)
AVCC3 | VCC 3 (main accelerator sensor)
AVCC4 | VCC 4 (sub accelerator sensor)
AVCCCRA | VCC (crank angle sensor)
AVCSEL+ | Exhaust cam angle sensor (L)
AVCSER+ | Exhaust cam angle sensor (R)
AVCSL+ | Intake cam angle sensor (L)
AVCSR+ | Intake cam angle sensor (R)
AVSS1 | VSS 1 (engine)
AVSS2 | VSS (air flow sensor)
AVSS3 | VSS 3 (main accelerator sensor)
AVSS4 | VSS 4 (sub accelerator sensor)
AVSSCAM | VSS (cam angle sensor)
AVSSCRA | VSS (crank angle sensor)
BATT | VB (back up)
BP | Brake vacuum sensor
BPRLY | Vacuum pressure vacuum pump relay
BRK1 | Brake SW 1 (cruise control cancel)
BRK2 | Brake SW 2 (stop light)
CAN2H | CAN 2 (H)
CAN2L | CAN 2 (L)
CAN3H | CAN 3 (H)
CAN3L | CAN 3 (L)
CANH | CAN 1 (H)
CANL | CAN 1 (L)
CCMD | Cruise control command SW
CLMAIN | Cruise control main SW
CLSTR | Clutch stroke sensor
CLTST1 | Clutch start SW 1
CLTST2 | Clutch start SW 2
CLTSW | Clutch SW (cruise control cancel)
CPC | CPC solenoid
CPC2 | CPC solenoid 2
CRADIGT | Crank angle sensor
CSO | Cam angle sensor output
CUTRM | Starter cut relay diagnosis input
DDC | DC/DC boost control
DDCVM | DC/DC voltage monitor
DELM | Delivery mode SW
EGR− | EGR motor (−)
EGR+ | EGR motor (+)
EGR1 | EGR #1
EGR2 | EGR #2
EGR3 | EGR #3
EGR4 | EGR #4
EGRS | EGR opening angle sensor
EHS1 | Hood SW
EHSDO | Hood SW diagnosis output
EREVOUT | Crank angle sensor output
FFLPRLY | Fuel flap relay
FFLPSW | Fuel flap status SW
FPC | FPC motor
FPCD | +B (fuel pump controller)
FPCDG | Fuel pump controller diagnosis input
FPH− | High-pressure fuel pump (−)
FPH+ | High-pressure fuel pump (+)
FPRLY | Fuel pump relay
FREQSW | Fuel request SW
FTPCV | Sealed valve output
FTPS | Fuel tank pressure sensor
FUELP1 | Fuel pressure sensor (main)
FUELP2 | Fuel pressure sensor (sub)
GNDBY | GND (body)
GNDEG1 | GND (engine 1)
GNDEG2 | GND (engine 2)
GNDEG3 | GND (engine 3)
GNDEG4 | GND (engine 4)
HB | Blower fan SW
HTFR1 | A/F heater
IGN1 | Ignition #1
IGN2 | Ignition #2
IGN3 | Ignition #3
IGN4 | Ignition #4
IMO1 | Immobilizer
INJ1− | D-INJ #1 (−)
INJ1+ | D-INJ #1 (+)
INJ2− | D-INJ #2 (−)
INJ2+ | D-INJ #2 (+)
INJ3− | D-INJ #3 (−)
INJ3+ | D-INJ #3 (+)
INJ4− | D-INJ #4 (−)
INJ4+ | D-INJ #4 (+)
KEY1 | IG SW 1
KEY2 | IG SW 2
KNKL | Knock sensor (L)
KNKL− | GND (knock sensor L)
KNKR | Knock sensor (R)
KNKR− | GND (knock sensor R)
KNKSLD | Shield (knock sensor)
LIN | LIN
LOADVBM | Vacuum pressure vacuum pump diagnosis input
MAP | Intake air pressure sensor
MPMP | ELCM motor
NEUT | Neutral SW 1
NEUT2 | Neutral SW 2
OCVEL | Exhaust AVCS solenoid L
OCVER | Exhaust AVCS solenoid R
OCVL | Intake AVCS solenoid L
OCVR | Intake AVCS solenoid R
OILP | Oil pressure sensor
OLEV | Oil level SW
PCVDG | PCV diagnosis input
PEG | GPF exhaust pressure difference sensor
PPMP | ELCM pressure sensor
REV− | MCV motor (−)
REV+ | MCV motor (+)
RFAN1 | Radiator fan relay 1
RFAN2 | Radiator fan relay 2
RFANC1 | Radiator fan control 1
RFANC2 | Radiator fan control 2
RFAND | +B (radiator fan controller)
RO2HR | Oxygen heater
RO2SR− | Oxygen sensor (−)
RO2SR+ | Oxygen sensor (+)
RSTA | Restart command
SSHUT | Self shut off relay
START | Starter SW
STCTRLY | Starter cut relay
STRLY | Starter relay
STRLY2 | Starter relay 2
STSW2 | Starter SW 2
TA | Intake air temperature sensor
TACHO | Engine speed signal
TGVLC | TGV L (close)
TGVLO | TGV L (open)
TGVRC | TGV R (close)
TGVRO | TGV R (open)
TGVSWL | TGV opening angle sensor (L)
TGVSWR | TGV opening angle sensor (R)
THEG1 | GPF exhaust temperature sensor (Fr)
THEG2 | GPF exhaust temperature sensor (Rr)
THEGDG | EGR temperature sensor
THM− | Throttle motor (−)
THM+ | Throttle motor (+)
THSM | Throttle sensor (main)
THSS | Throttle sensor (sub)
THSSLD | Shield (throttle sensor)
TO | Oil temperature sensor
TPS− | VSS (throttle sensor)
TPS5V | VCC (throttle sensor)
TW | Engine coolant temperature sensor
TW IN | Engine coolant temperature sensor IN
TW OUT | Engine coolant temperature sensor OUT
TW3 | Engine coolant temperature sensor 3
VBEC1 | VB (control 1)
VBEC2 | VB (control 2)
VPMP | ELCM switching valve

13. KEYLESS ACCESS CM

Abbr. | Full name
+B1 | +B power supply (main)
+B2 | +B power supply (DCDC)
ACCD | ACC relay drive requirement
ACCR | ACC cut input
AGND | Immobilizer amplifier GND
BZR | Buzzer output circuit
CANL | Can communication (L)
CG1B | D seat exterior antenna (−)
CG2B | P seat exterior antenna (−)
CG5B | Front interior antenna (−)
CG6B | Rear interior antenna (−)
CG7B | Inner cargo room antenna (−)
CG8B | Rear exterior antenna (−)
CHAH | Can communication (H)
CLG1 | D seat exterior antenna (+)
CLG2 | P seat exterior antenna (+)
CLG5 | Front interior antenna (+)
CLG6 | Rear interior antenna (+)
CLG7 | Inner cargo room antenna (+)
CLG8 | Rear exterior antenna (+)
CLUT | Clutch input
CODE | Immobilizer signal reception (start SW)
EGIO | Immobilizer verification communication wire
GND1 | GND 1
GND2 | GND 2
IDW | With/without id code box judgement
IG1D | IG 1 relay drive output
IG2D | IG 2 relay drive output
INDS | Indicator output (green)
INDW | Indicator output (orange)
LIN | LIN communication
P | Shift p position input
SLP | Steering lock position input
SLR+ | Steering lock motor power supplying signal output
SPD | Vehicle speed
SSW 1 | Start switch input 1
SSW2 | Start switch input 2
STP1 | Stop lamp SW input
STSW | Starter drive requirement output
SWIL | Start SW letter lighting
TACH | Engine speed
TSW5 | Request switch input
TXCT | Immobilizer signal reception (start SW)
VC5 | Immobilizer amplifier power supply
WPC | Wireless charger stop request signal output circuit

14. KEYLESS ENTRY CM

Abbr. | Full name
+B | Battery power supply
CANH | CAN-H
CANL | CAN-L
GND | GND
IGN | Ignition power supply
SET | TPMS set switch connection

15. MFD (STANDARD MFD)

Abbr. | Full name
+B | +B power supply
GND | GND
IGN | +IGN power supply
MFD SW+ | MFD operation SW input
U-ART | UART Input

16. MFD (HIGH GRADE MFD)

Abbr. | Full name
+B | +B power supply
+IGN | +IGN power supply
5V | USB power supply
CAMERA SW1+ | Camera SW 1 (+)
CAMERA SW2+ | Camera SW 2 (+)
CAN− | CAN (−)
CAN+ | CAN (+)
DATA− | USB interface signal (−)
DATA+ | USB interface signal (+)
GND | GND
USB GND
MFD SW+ | MFD operation SW input
OUTREQ | External video 2 output request
External video 1 output request
POWER | External video 2 power supply
External video 1 power supply
U-ART | UART Input
VIDEO− | External video 2 connection detection
External video 1 connection detection
VIDEO+ | External video 2 NTSC video signal
External video 1 NTSC video signal

17. OCCUPANT DETECTION CM

Abbr. | Full name
+B | Battery power supply
BER− | Buckle switch GND
BER+ | Buckle switch signal
FSR− | GND
FSR+ | A/B ECM communication line
IG | IG switch
SGD1 | Load sensor 1 (FL) GND
SGD2 | Load sensor 2 (FR) GND
SGD3 | Load sensor 3 (RL) GND
SGD4 | Load sensor 4 (RR) GND
SIG1 | Load sensor 1 (FL) signal
SIG2 | Load sensor 2 (FR) signal
SIG3 | Load sensor 3 (RL) signal
SIG4 | Load sensor 4 (RR) signal
SVC1 | Load sensor 1 (FL) power supply
SVC2 | Load sensor 2 (FR) power supply
SVC3 | Load sensor 3 (RL) power supply
SVC4 | Load sensor 4 (RR) power supply

18. POWER REAR GATE CM

Abbr. | Full name
+B | Battery power supply (ECM)
+POWER B | Battery power supply (power system)
APS | Touch sensor
BUZ (+) | Buzzer (+)
BUZ RTN (−) | Buzzer (−)
CLOSER (CLOSE) | Closer motor close output
CLOSER (OPEN) | Closer motor open output
COURTESY SW | Courtesy switch
DR SW | Power rear gate driver's seat SW
ECU GND | ECM GND
HALL 1 | Hall (pulse) 1
HALL 2 | Hall (pulse) 2
HALL FEED | Hall feed
HALL RTN | Hall return
HAZARD OUT | Hazard output
IGN SW | Ignition switch
LATCH SW | Latch switch
LIN | LIN communication
MEM SW | Memory height switch
PRG MOTOR (CLOSE) | Power rear gate motor close output
PRG MOTOR (OPEN) | Power rear gate motor open output
RATCHET SW | Ratchet switch
RG INR SW | R/G inner SW
SECTOR SW | Sector switch
SW GND | Switch GND

19. POWER SEAT & REMOTE CONTROL MIRROR CM

Abbr. | Full name
ACC | ACC power supply
BMR | Mirror load operation power supply
BSE | Seat motor drive power supply
CLR | Electric retractable SW input (retract)
CPUB | ECM power supply
GND1 | ECM GND
GND2
IG | Ignition power supply
LE | LH mirror memory sensor GND
LFT− | Lifter motor (−)
LFT +SW | Lifter switch (+)
LFT SEN | Lifter pulse
LFT −SW | Lifter switch (−)
LFT+ | Lifter motor (+)
LHSSR | LH mirror memory sensor input (right/left)
LIN | LIN communication
LM+ | LH mirror mirror face output (+)
LMH | LH mirror mirror face output (right/left)
LMR− | LH mirror electric retractable motor (−)
LMR+ | LH mirror electric retractable motor (+)
LMV | LH mirror mirror face output (up/down)
LVC | LH mirror memory sensor power supply
LVSSR | LH mirror memory sensor input (up/down)
M1 | Memory 1
M2 | Memory 2
M3 | Memory 3
MAL | Remote control mirror SW MAL input (LH)
MAR | Remote control mirror SW MAL input (RH)
MBL | Remote control mirror SW MBL input (LH)
MBR | Remote control mirror SW MBL input (RH)
MCL | Remote control mirror SW MCL input (LH)
MRE | Mirror SW GND
MRS | Remote control mirror SW power supply
OPR | Electric retractable SW input (extend)
RCL− | Reclining motor (−)
RCL +SW | Reclining switch (+)
RCL SEN | Reclining pulse
RCL −SW | Reclining switch (−)
RCL+ | Reclining motor (+)
RE | RH mirror memory sensor GND
RHSSR | RH mirror memory sensor input (right/left)
RM+ | RH mirror mirror face motor output (+)
RMH | RH mirror mirror face motor output (right/left)
RMR− | RH mirror electric retractable motor output (−)
RMR+ | RH mirror electric retractable motor output (+)
RMV | RH mirror mirror face motor output (up/down)
RVC | RH mirror memory sensor power supply
RVSSR | RH mirror memory sensor input (up/down)
SET | Memory set
SG | Seat pulse sensor GND
SLD− | Slide motor (−)
SLD +SW | Slide switch (+)
SLD SEN | Slide pulse
SLD −SW | Slide switch (−)
SLD+ | Slide motor (+)
TLT− | Tilt motor (−)
TLT +SW | Tilt switch (+)
TLT SEN | Tilt pulse
TLT −SW | Tilt switch (−)
TLT+ | Tilt motor (+)
VCC | Seat motor pulse sensor power supply

20. POWER STEERING CM

Abbr. | Full name
BATT | Battery power supply
CAN-H | CAN-H
CAN-L | CAN-L
GND | GND
IGN SW | Ignition power supply

21. RAB CM

Abbr. | Full name
+B | Battery power supply
CAN0_H | Main CAN (High)
CAN0_L | Main CAN (Low)
CAN1_H | Local CAN (High)
CAN1_L | Local CAN (Low)
GND | GND
IGN | Ignition power supply
RL− | Left corner sensor (−)
RL+ | Left corner sensor (+)
RLC− | Left inner sensor (−)
RLC+ | Left inner sensor (+)
RR− | Right corner sensor (−)
RR+ | Right corner sensor (+)
RRC− | Right inner sensor (−)
RRC+ | Right inner sensor (+)

22. RADAR SENSOR LH

Abbr. | Full name
BSM ICON | BSD/RCTA indicator (LH)
BSM MAIN | BSD/RCTA ON/OFF SW
GND | GND
IG1 | Ignition power supply
MS CAN H | Main CAN (High)
MS CAN L | Main CAN (Low)
PRI CAN H | BSD/RCTA local CAN (High)
PRI CAN L | BSD/RCTA local CAN (Low)

23. RADAR SENSOR RH

Abbr. | Full name
BSM ICON | BSD/RCTA indicator (RH)
GND | GND
IG1 | Ignition power supply
PRI CAN H | BSD/RCTA local CAN (High)
PRI CAN L | BSD/RCTA local CAN (Low)

24. REAR SEAT HEATER CM

Abbr. | Full name
+B | Seat heater drive power supply
GND | GND
IG | ECM power supply
RL INDH | RL position indicator drive output (HI)
RL INDL | RL position indicator drive output (LO)
RL SW | RL position seat heater sw input
RLB | RL position seat back heater GND
RLC | RL position seat cushion heater GND
RLH | RL position seat heater drive output
RR INDH | RR position indicator drive output (HI)
RR INDL | RR position indicator drive output (LO)
RR SW | RR position seat heater sw input
RRB | RR position seat back heater GND
RRC | RR position seat cushion heater GND
RRH | RR position seat heater drive output

25. STEERING LOCK CM

Abbr. | Full name
B | Battery power supply
GND | GND
IGN1 | Ignition power supply
LIN | LIN communication
SLP | Unlock position output
SLR+ | Steering lock motor drive power supply

26. STEREO CAMERA

Abbr. | Full name
CAN-H | CAN-H
CAN-L | CAN-L
CAN-R-H | Local CAN-H (RAB communication line)
CAN-R-L | Local CAN-L (RAB communication line)
CRU-SW1 | EyeSight steering switch input
CRU-SW2
DEBUG(SCI-RX) | Serial RX for development
DEBUG(SCI-TX) | Serial TX for development
GND1 | GND
GND-CRU-SW | EyeSight steering switch GND
IGN | Ignition power supply
LW-OFF-SW | Lane departure warning OFF switch input
PB-OFF-SW | Pre-collision brake OFF switch input
RLY-CNT | Brake light relay
VB | Battery power supply

27. SUNROOF UNIT

Abbr. | Full name
12V | Battery power supply
GND | GND
IGN | Ignition power supply
LIN | LIN communication
SW2 | Slide open switch input
SW3 | Slide close switch input

28. TCM

Abbr. | Full name
AWD DUTY SOL | AWD duty SOL
B/U PWR | Backup power supply
CAN− | CAN (−)
CAN+ | CAN (+)
D RNG SW | D range SW
DN SW | Down SW
EOP COM | Electric fluid pump operation command signal
EOP OPE | Electric fluid pump operation status signal
EOP RLY | Electric fluid pump relay drive
F/R LIN SOL | F/R linear SOL
GND 1 | TCM GND 1
GND 2 | TCM GND 2
IGSW | IGSW signal
L/M MODE SW | LO/manual mode SW
L/U DUTY SOL | Lock-up duty solenoid
MAIN PWR 1 | Main power supply 1
MAIN PWR 2 | Main power supply 2
MAIN PWR 3 | Main power supply 3
N RNG SW | N range SW
OIL PRS SSR GND | GND dedicated for oil pressure sensor
OIL PRS SSR PWR | Oil pressure sensor power supply
OIL PRS SSR SIG | Oil pressure sensor signal
OIL TEMP SSR GND | GND dedicated for oil temperature sensor
OIL TEMP SSR SIG | Oil temperature sensor signal
P RNG SW | P range SW
PRI DN DUTY SOL | Primary discharge duty SOL
PRI SPD SSR | Primary speed sensor
PRI UP DUTY SOL | Primary supply duty SOL
R RNG SW | R range SW
SEC PRS LIN SOL | Secondary pressure linear SOL
SEC SPD SSR | Secondary speed sensor
STAT COM | Start command circuit
STP SW | Stop light SW
STR SW | Starter SW
TUR SPD SSR | Turbine speed sensor
UP SW | Up SW
VPP | VPP

29. TPMS & KEYLESS ENTRY CM

Abbr. | Full name
+B | Battery power supply
CANH | CAN-H
CANL | CAN-L
GND | GND
IGN | Ignition power supply
SET | TPMS set switch connection

30. TPMS CM

Abbr. | Full name
+B | Battery power supply
CANH | CAN-H
CANL | CAN-L
GND | GND
IGN | Ignition power supply
SET | TPMS set switch connection

31. VDC CM

Abbr. | Full name
AVH SW | Auto vehicle hold switch
BLA | Stop light switch output
BLS | Stop light switch
CAN_H | CAN-H
CAN_L | CAN-L
EPB L A(+) | LH rear brake caliper (+)
EPB L B(−) | LH rear brake caliper (−)
EPB R A(+) | RH rear brake caliper (+)
EPB R B(−) | RH rear brake caliper (−)
FL_GND (WSS) | FL wheel speed sensor GND
FL_SIG (WSS) | FL wheel speed sensor signal
FLUID LEVEL | Brake fluid level switch
FR_GND (WSS) | FR wheel speed sensor GND
FR_SIG (WSS) | FR wheel speed sensor signal
GND | Ground
GND_MR
IGN | Ignition power supply
IND (EPB SW) | Electronic parking brake indicator light
RL_GND (WSS) | RL wheel speed sensor GND
RL_SIG (WSS) | RL wheel speed sensor signal
RR_GND (WSS) | RR wheel speed sensor GND
RR_SIG (WSS) | RR wheel speed sensor signal
SENT | Brake booster pressure sensor signal
SENT GND | Brake booster pressure sensor GND
SW 1 (EPB SW) | Electronic parking brake switch
SW 2 (EPB SW)
SW 3 (EPB SW)
SW 4 (EPB SW)
UVMR | VDC pump motor power supply
UVVR | VDC CM power supply
VCC | Brake booster pressure sensor power supply
VDC OFF | VDC OFF switch
VSO | VSO PIN output

WIRING SYSTEM > Harness Repair Kit
SPECIFICATION
1. APPLICATION CHART
WIRING SYSTEM > Fuse And Relay
LOCATION
1. ENGINE COMPARTMENT SIDE
2. PASSENGER ROOM SIDE
WIRING SYSTEM > Power Supply Circuit
WIRING DIAGRAM
1. WITHOUT PUSH BUTTON START

No. | Load
MB-1 | Blower motor relay
MB-2 | OP connector (power amplifier)
MB-3 | DC/DC converter 1
MB-4 | DC/DC converter 1
MB-5 | VDC CM
MB-6 | VDC CM
MB-7 | Wiper deicer relay
MB-8 | DC/DC converter 2
MB-9 | Rear defogger relay
MB-10 | Active grille shutter
Front fog light relay
MB-11 | Main fan relay 1
MB-12 | Sub fan relay
MB-13 | Combination switch
Front wiper motor
MB-14 | Front washer motor
MB-15 | Rear wiper relay
Rear washer motor
Rear wiper motor
MB-16 | Power steering CM
MB-17 | Data link connector
MB-18 | Battery sensor
ECM
TCM
MB-19 | Battery sensor
Electric fluid pump relay
MB-20 | Horn LH
MB-21 | Horn RH
MB-22 | Horn switch
Body integrated unit
MB-23 | Starter cut relay
MB-24 | EGR control valve
Exhaust camshaft position sensor LH
Exhaust camshaft position sensor RH
Intake camshaft position sensor LH
Intake camshaft position sensor RH
Leak check valve ASSY
Purge control solenoid valve
MB-26 | Exhaust oil control solenoid LH
Exhaust oil control solenoid RH
Intake oil control solenoid LH
Intake oil control solenoid RH
MB-27 | Front oxygen (A/F) sensor
Rear oxygen sensor
MB-28 | Ignition coil No. 1
Ignition coil No. 2
Ignition coil No. 3
Ignition coil No. 4
MB-29 | ECM
MB-31 | TCM
MB-32 | Primary speed sensor
Secondary speed sensor
Turbine speed sensor
MB-33 | ECM
MB-34 | Fuel pump relay
MB-35 | Front combination light RH
MB-36 | Front combination light LH
MB-37 | Body integrated unit
Daytime running light relay
MB-38 | Body integrated unit
MB-39 | Power window circuit breaker
MB-41 | Data communication module
MB-42 | AUX input terminal (instrument panel)
MB-51 | Airbag CM
Occupant detection CM
MB-52 | Body integrated unit
MB-53 | Body integrated unit
MB-54 | Body integrated unit
MB-55 | Body integrated unit
ACC-1 | OP connector (remote engine start CM)
IG-1 | OP connector (remote engine start CM)
ST-1 | ECM
OP connector (remote engine start CM)
TCM
SB-1 | Body integrated unit
SB-2 | Body integrated unit
Rear gate unlock relay
Front unlock relay
Front lock relay
FB-1 | Stop light & brake switch
Stop light relay
FB-3 | Steering heater/Seat heater relay
FB-5 | OP connector (trailer)
FB-6 | A/C control panel
FB-8 | Body integrated unit
FB-9 | AVH/EPB control switch
Keyless entry CM
TPMS & keyless entry CM
Power rear gate CM
FB-10 | Combination meter
FB-11 | Air mix door actuator (without L/R independent air conditioner)
Air mix door actuator RH (with L/R independent air conditioner)
Air mix door actuator LH
Mode door actuator
FB-13 | Immobilizer CM
FB-14 | Auto headlight beam leveler CM
FB-15 | A/C control panel
FB-16 | Audio/Navigation unit
FB-19 | Front door step light RH
Outer mirror ASSY RH
FB-20 | Immobilizer antenna
FB-21 | Front door step light LH
Outer mirror ASSY LH
FB-22 | Luggage room light
Power rear gate inner switch
FB-23 | Room light
Spot map light
Vanity mirror light LH
Vanity mirror light RH
Warning box
FB-25 | Combination meter
MFD
FB-26 | Radar sensor LH (master)
Radar sensor RH (slave)
RAB CM
Shift position indicator
FB-27 | Stereo camera
Warning box
FB-28 | A/C control panel
FB-30 | Key warning switch
OP connector (remote engine start CM)
FB-31 | Body integrated unit
FB-32 | MFD
FB-36 | OP connector (remote engine start CM)
FB-37 | RAB CM
Stereo camera
FB-38 | OP connector (rearview mirror)
Remote control mirror switch
FB-39 | Front accessory power supply socket
Rear accessory power supply socket (cargo room)
FB-40 | Rear accessory power supply socket (console)
FB-41 | Daytime running light relay
FB-43 | Blower motor relay
FB-44 | Data communication module
FB-45 | Rear defogger relay
Sub fan relay
Wiper deicer relay
FB-46 | Keyless entry CM
Power rear gate CM
TPMS & keyless entry CM
FB-47 | BSD/RCTA OFF switch
Data link connector
FB-48 | Sunroof unit
FB-49 | Stop light & brake switch
FB-50 | Immobilizer CM
Power window relay
FB-51 | Main fan relay 1
Main fan relay 2
FB-52 | AVH/EPB control switch
FB-53 | Auto headlight beam leveler CM
Front combination light LH
Front combination light RH
Inhibitor switch
FB-54 | Audio/Navigation unit
Audio amplifier
Data communication module
USB power supply (console)
FB-56 | Steering heater/Seat heater relay
FB-57 | DC/DC converter 1
FB-58 | Stop light relay
VDC CM
FB-59 | Steering angle sensor
FB-60 | Power steering CM
FB-63 | Airbag CM
FB-64 | Occupant detection CM
FB-66 | DC/DC converter 1
DC/DC converter 2
FB-67 | ECM
Fuel pump relay
Starter cut relay
Starter relay
TCM

2. WITH PUSH BUTTON START

No. | Load
MB-1 | Blower motor relay
MB-2 | OP connector (power amplifier)
MB-3 | DC/DC converter 1
MB-4 | DC/DC converter 1
MB-5 | VDC CM
MB-6 | VDC CM
MB-7 | Wiper deicer relay
MB-8 | DC/DC converter 2
MB-9 | Rear defogger relay
MB-10 | Active grille shutter
Front fog light relay
MB-11 | Main fan relay 1
MB-12 | Sub fan relay
MB-13 | Combination switch
Front wiper motor
MB-14 | Front washer motor
MB-15 | Rear wiper relay
Rear washer motor
Rear wiper motor
MB-16 | Power steering CM
MB-17 | Data link connector
MB-18 | Battery sensor
ECM
TCM
MB-19 | Battery sensor
Electric fluid pump relay
MB-20 | Horn LH
MB-21 | Horn RH
MB-22 | Horn switch
Body integrated unit
MB-23 | Starter cut relay
MB-24 | EGR control valve
Exhaust camshaft position sensor LH
Exhaust camshaft position sensor RH
Intake camshaft position sensor LH
Intake camshaft position sensor RH
Leak check valve ASSY
Purge control solenoid valve
MB-26 | Exhaust oil control solenoid LH
Exhaust oil control solenoid RH
Intake oil control solenoid LH
Intake oil control solenoid RH
MB-27 | Front oxygen (A/F) sensor
Rear oxygen sensor
MB-28 | Ignition coil No. 1
Ignition coil No. 2
Ignition coil No. 3
Ignition coil No. 4
MB-29 | ECM
MB-31 | TCM
MB-32 | Primary speed sensor
Secondary speed sensor
Turbine speed sensor
MB-33 | ECM
MB-34 | Fuel pump relay
MB-35 | Front combination light RH
MB-36 | Front combination light LH
MB-37 | Body integrated unit
Daytime running light relay
MB-38 | Body integrated unit
MB-39 | Power window circuit breaker
MB-41 | Data communication module
MB-42 | AUX input terminal (instrument panel)
MB-50 | Remote control back rest switch LH
Remote control back rest switch RH
MB-51 | Airbag CM
Occupant detection CM
MB-52 | Body integrated unit
MB-53 | Body integrated unit
MB-54 | Body integrated unit
MB-55 | Body integrated unit
MB-56 | Rear seat heater CM
SB-1 | Body integrated unit
SB-2 | Body integrated unit
Rear gate unlock relay
Front unlock relay
Front lock relay
FB-1 | Stop light & brake switch
Stop light relay
FB-3 | Steering heater/Seat heater relay
FB-5 | OP connector (trailer)
FB-6 | A/C control panel
FB-7 | Keyless access CM
FB-8 | Body integrated unit
FB-9 | AVH/EPB control switch
TPMS CM
Power rear gate CM
Power seat & remote control mirror CM
FB-10 | Combination meter
FB-11 | Air mix door actuator (without L/R independent air conditioner)
Air mix door actuator RH (with L/R independent air conditioner)
Air mix door actuator LH
Mode door actuator
FB-14 | Auto headlight beam leveler CM
FB-15 | A/C control panel
FB-16 | Audio/Navigation unit
FB-19 | Front door step light RH
Outer mirror ASSY RH
FB-20 | OP connector (remote engine start CM)
FB-21 | Front door step light LH
Outer mirror ASSY LH
FB-22 | Luggage room light
Power rear gate inner switch
Power rear gate lock button
Rear gate light
FB-23 | Room light
Spot map light
Vanity mirror light LH
Vanity mirror light RH
Warning box
FB-25 | Combination meter
MFD
FB-26 | Radar sensor LH (master)
Radar sensor RH (slave)
RAB CM
Shift position indicator
FB-27 | Stereo camera
Warning box
FB-28 | A/C control panel
FB-30 | ID code box
Keyless access CM
Steering lock CM
FB-31 | Body integrated unit
FB-32 | MFD
FB-37 | Driver monitoring unit
RAB CM
Stereo camera
FB-38 | OP connector (rearview mirror)
Remote control mirror switch
FB-39 | Front accessory power supply socket
Rear accessory power supply socket (cargo room)
FB-40 | Rear accessory power supply socket (console)
FB-41 | Daytime running light relay
FB-42 | Steering lock CM
FB-43 | Blower motor relay
FB-44 | Data communication module
Rear seat heater CM
FB-45 | Rear defogger relay
Sub fan relay
Wiper deicer relay
FB-46 | Power rear gate CM
Power seat & remote control mirror CM
TPMS CM
FB-47 | BSD/RCTA OFF switch
Data link connector
OP connector (remote engine start CM)
FB-48 | Sunroof unit
FB-49 | Stop light & brake switch
FB-50 | Power window relay
FB-51 | Main fan relay 1
Main fan relay 2
FB-52 | AVH/EPB control switch
FB-53 | Auto headlight beam leveler CM
Front combination light LH
Front combination light RH
Inhibitor switch
FB-54 | Audio/Navigation unit
Audio amplifier
Data communication module
USB power supply (console)
FB-55 | Power seat & remote control mirror CM
FB-56 | Body integrated unit
Steering heater/Seat heater relay
FB-57 | DC/DC converter 1
FB-58 | Stop light relay
VDC CM
FB-59 | Steering angle sensor
FB-60 | Power steering CM
FB-63 | Airbag CM
FB-64 | Occupant detection CM
FB-66 | DC/DC converter 1
DC/DC converter 2
FB-67 | ECM
Fuel pump relay
Starter cut relay
Starter relay
TCM

WIRING SYSTEM > Ground Circuit
WIRING DIAGRAM
WIRING SYSTEM > Active Grille Shutter
WIRING DIAGRAM
WIRING SYSTEM > Airbag System
WIRING DIAGRAM
WIRING SYSTEM > Air Conditioning System
WIRING DIAGRAM
WIRING SYSTEM > Audio and Navigation System
WIRING DIAGRAM
1. WITHOUT AUDIO AMPLIFIER, WITHOUT TELEMATICS
2. WITH AUDIO AMPLIFIER, WITHOUT TELEMATICS
3. WITHOUT AUDIO AMPLIFIER, WITH TELEMATICS
4. WITH AUDIO AMPLIFIER, WITH TELEMATICS
WIRING SYSTEM > Auto Start Stop
WIRING DIAGRAM
WIRING SYSTEM > Back-up Light System
WIRING DIAGRAM
WIRING SYSTEM > Blind Spot Detection/Rear Cross Traffic Alert
WIRING DIAGRAM
WIRING SYSTEM > CAN Communication System
WIRING DIAGRAM
WIRING SYSTEM > Charging System
WIRING DIAGRAM
WIRING SYSTEM > Clearance Light and Illumination Light System
WIRING DIAGRAM
WIRING SYSTEM > Combination Meter System
WIRING DIAGRAM
1. NORMAL METER MODEL
2. COLOR TFT METER MODEL
WIRING SYSTEM > Cruise Control System
WIRING DIAGRAM
WIRING SYSTEM > CVT Control System
WIRING DIAGRAM
WIRING SYSTEM > Daytime Running Light System
WIRING DIAGRAM
1. WITHOUT SRH
2. WITH SRH
WIRING SYSTEM > Door Lock Control System
WIRING DIAGRAM
WIRING SYSTEM > Driver Monitoring System
WIRING DIAGRAM
WIRING SYSTEM > Electric Power Steering System
WIRING DIAGRAM
WIRING SYSTEM > Engine Electrical System
WIRING DIAGRAM
1. WITHOUT PUSH BUTTON START
2. WITH PUSH BUTTON START
WIRING SYSTEM > EyeSight System
WIRING DIAGRAM
WIRING SYSTEM > Front Accessory Power Supply Socket System
WIRING DIAGRAM
WIRING SYSTEM > Front Fog Light System
WIRING DIAGRAM
WIRING SYSTEM > Front Wiper and Washer System
WIRING DIAGRAM
WIRING SYSTEM > Headlight Beam Leveler System
WIRING DIAGRAM
WIRING SYSTEM > Headlight System
WIRING DIAGRAM
WIRING SYSTEM > Horn System
WIRING DIAGRAM
WIRING SYSTEM > Immobilizer System
WIRING DIAGRAM
1. WITHOUT PUSH BUTTON START
2. WITH PUSH BUTTON START

WIRING SYSTEM>Keyless Access With Push Button Start System>WIRING DIAGRAM

WIRING SYSTEM > Interior Light System
WIRING DIAGRAM
WIRING SYSTEM > Keyless Access With Push Button Start System
WIRING DIAGRAM
WIRING SYSTEM > Keyless Entry System
WIRING DIAGRAM
WIRING SYSTEM > Multi-function Display (MFD) System
WIRING DIAGRAM
1. STANDARD MFD
2. HIGH GRADE MFD
WIRING SYSTEM > Occupant Detection System
WIRING DIAGRAM
WIRING SYSTEM > Parking Brake / Brake Fluid Level Warning Light System
WIRING DIAGRAM
WIRING SYSTEM > Power Rear Gate System
WIRING DIAGRAM
WIRING SYSTEM > Power Seat System
WIRING DIAGRAM
1. WITHOUT SEAT POSITION MEMORY
2. WITH SEAT POSITION MEMORY
WIRING SYSTEM > Power Window System
WIRING DIAGRAM
1. WITH DRIVER'S SEAT ONLY OFF DELAY FUNCTION
2. WITH FRONT SEATS ONLY OFF DELAY FUNCTION
3. WITH ALL SEATS OFF DELAY FUNCTION
WIRING SYSTEM > Radiator Fan System
WIRING DIAGRAM
WIRING SYSTEM > Rear Accessory Power Supply Socket System
WIRING DIAGRAM
WIRING SYSTEM > Rear Defogger System
WIRING DIAGRAM
WIRING SYSTEM > Rearview Camera System
WIRING DIAGRAM
WIRING SYSTEM > Rearview Mirror System
WIRING DIAGRAM
WIRING SYSTEM > Rear Wiper and Washer System
WIRING DIAGRAM
WIRING SYSTEM > Remote Control Back Rest System
WIRING DIAGRAM
WIRING SYSTEM > Remote Control Mirror System
WIRING DIAGRAM
1. WITHOUT SEAT POSITION MEMORY
2. WITH SEAT POSITION MEMORY
WIRING SYSTEM > Remote Engine Start System
WIRING DIAGRAM
1. WITHOUT PUSH BUTTON START
2. WITH PUSH BUTTON START
WIRING SYSTEM > Reverse Automatic Braking
WIRING DIAGRAM
WIRING SYSTEM > Seat Heater System
WIRING DIAGRAM
1. FRONT SEAT
2. REAR SEAT
WIRING SYSTEM > Security System
WIRING DIAGRAM
WIRING SYSTEM > Shift Lock Control System
WIRING DIAGRAM
WIRING SYSTEM > Starter System
WIRING DIAGRAM
WIRING SYSTEM > Steering Heater System
WIRING DIAGRAM
WIRING SYSTEM > Stop Light System
WIRING DIAGRAM
WIRING SYSTEM > Sunroof Control System
WIRING DIAGRAM
WIRING SYSTEM > Telematics System
WIRING DIAGRAM
1. WITHOUT AUDIO AMPLIFIER
2. WITH AUDIO AMPLIFIER
WIRING SYSTEM > Tire Pressure Monitoring System
WIRING DIAGRAM
WIRING SYSTEM > Trailer Hitch Connector System
WIRING DIAGRAM
WIRING SYSTEM > Turn Signal Light and Hazard Light System
WIRING DIAGRAM
WIRING SYSTEM > Vehicle Dynamics Control System
WIRING DIAGRAM
WIRING SYSTEM > Wiper Deicer System
WIRING DIAGRAM
WIRING SYSTEM > Harness Components Location
LOCATION

(1) | Front wiring harness | (9) | Roof cord | (17) | Occupant detection wiring harness
(2) | Engine wiring harness | (10) | Rear gate cord LWR | (18) | Stereo camera cover adapter cord
(3) | Bulkhead wiring harness | (11) | Rear gate cord UPR | (19) | Sonar sensor cord
(4) | Instrument panel wiring harness | (12) | Rear door cord LH | (20) | Adapter cord (AUX)
(5) | Front door cord RH | (13) | Front door cord LH | (21) | Adapter cord (console)
(6) | Rear door cord RH | (14) | Transmission cord | (22) | Parking brake sub wiring harness RH
(7) | Rear wiring harness RH | (15) | Electrical power steering harness | (23) | Parking brake sub wiring harness LH
(8) | Rear wiring harness LH | (16) | Power seat wiring harness

WIRING SYSTEM > Front Wiring Harness
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
F25 | ― | ― | B-3 |  | Generator terminal B
F26 | 1 | B | C-3 |  | Generator
F135 | 11 | Gr | B-5 | E127 | Engine wiring harness
F160 | 2 | Gr | C-4 |  | Compressor solenoid
F162 | 1 | B | B-5 |  | Starter motor
F165 | 1 |  | B-5 |  | Battery cable
：White or natural color

WIRING SYSTEM > Bulkhead Wiring Harness (In Engine Compartment) RH
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB16 | 2 | B | C-2 |  | Front impact sensor RH
B3 | 4 | B | B-3 |  | Mass air flow & intake air temperature sensor
B6 | 2 | Gr | B-3 |  | Front ABS wheel speed sensor RH
B44 | 1 | B | C-2 |  | Horn LH
B203 | 3 | Br | B-4 | B204 | Electrical power steering harness
B204 | 3 | Br | B-4 | B203 | Bulkhead wiring harness
B205 | 2 | Gr | B-4 | B206 | Electrical power steering harness
B206 | 2 | Gr | B-4 | B205 | Bulkhead wiring harness
B225 | 60 | B | B-2 |  | Relay holder
B310 | 46 | B | B-3 |  | VDC CM
B329 | 3 | B | C-3 |  | Hood switch
B450 | 10 | B | C-4 |  | Power steering CM
B452 | 2 | B | C-4 |
B482 | 2 | Gr | C-3 |  | Sub fan motor
B486 | 6 | Gr | C-2 | B628 | Short connector
B487 | 8 | Gr | C-2 |  | Front combination light RH (without SRH)
10 | Gr | C-2 |  | Front combination light RH (with SRH)
B488 | 2 | B | C-1 |  | Front fog light RH
B489 | 1 | B | C-1 |  | Horn RH
B620 | 6 | B | C-2 |  | Front combination light RH
B628 | 6 | Gr | D-2 | B486 | Short connector
B638 | 10 | B | B-4 |  | J/C
B640 | 2 | B | D-2 |  | Ambient sensor
GV | ― | ― | B-3 |  | ―
GAP | ― | ― | B-4 |
GB-9 | ― | ― | C-2 |
：White or natural color

WIRING SYSTEM > Bulkhead Wiring Harness (In Engine Compartment) LH
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB13 | 2 | B | C-3 |  | Front impact sensor LH
B8 | 5 | Gr | A-4 |  | Front wiper motor
B9 | 3 | B | B-4 |  | Battery sensor
B15 | 2 | Gr | D-1 |  | Front ABS wheel speed sensor LH
B16 | 2 | Gr | B-4 |  | Brake fluid level switch
B19 | 4 | B | C-3 |  | Rear oxygen sensor
B63 | 4 | B | D-3 |  | Active grille shutter
B134 | 72 | B | B-4 |  | ECM
B138 | 10 | B | D-2 |  | J/C
B139 | 76 |  | D-2 | E3 | Engine wiring harness
B146 | 2 | Gr | D-4 |  | Front washer motor
B147 | 2 | Gr | D-4 |  | Rear washer motor
B177 | 2 | Gr | A-1 |  | Wiper deicer
B379 | 4 | Gr | D-2 |  | Front oxygen (A/F) sensor
B396 | 2 | B | D-4 |  | Washer fluid level sensor
B473 | 2 | Gr | C-3 |  | Main fan motor
B474 | 2 | B | D-4 |  | Front fog light LH
B477 | 8 | Gr | C-4 |  | Front combination light LH (without SRH)
10 | Gr | C-4 |  | Front combination light LH (with SRH)
B490 | 2 | Gr | C-4 |  | Keyless buzzer
B565 | 3 | Gr | B-4 |  | Brake booster pressure sensor
B621 | 6 | B | C-3 |  | Front combination light LH
B622 | 3 | Gr | D-3 | B623 | Short connector
B623 | 3 | Gr | D-3 | B622
B626 | 3 | B | C-3 |  | Pressure sensor (PD)
B627 | 3 | B | C-3 |  | Pressure sensor (PH)
B635 | 10 | B | B-4 |  | J/C
GB-1 | ― | ― | D-1 |  | ―
GB-10 | ― | ― | C-3 |
：White or natural color

WIRING SYSTEM > Bulkhead Wiring Harness (In Compartment)
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
B41 | 2 |  | C-1 |  | Power window circuit breaker
B49 | 4 | Y | C-3 | i115 | Instrument panel wiring harness
B52 | 4 |  | B-2 |  | F/B
B56 | 8 | Br | C-2 |
B60 | 86 |  | C-2 | i112 | Instrument panel wiring harness
B65 | 5 |  | C-4 |  | Stop light & brake switch
B129 | 18 |  | B-2 | i215 | Instrument panel wiring harness
B130 | 6 |  | B-3 | i216
B152 | 4 | B | B-2 |  | F/B
B158 | 20 |  | B-2 |
B159 | 4 |  | C-2 |
B180 | 4 |  | B-2 |  | OP connector (remote engine start CM)
B181 | 2 |  | B-3 | B182 | Short connector
B182 | 2 |  | B-3 | B181
B280 | 12 | B | C-2 |  | Body integrated unit
B281 | 20 | Gr | C-2 |
B287 | 8 |  | C-2 |
B315 | 6 | B | C-5 |  | Accelerator pedal position sensor
B491 | 5 |  | C-1 |  | J/C
B562 | 14 | Gr | C-3 |  | DC/DC converter 1
B563 | 5 |  | C-3 |
B616 | 16 |  | B-4 |  | Auto headlight beam leveler CM
B619 | 22 | B | B-1 |  | J/C
B629 | 6 |  | C-3 |  | DC/DC converter 2
B630 | 4 |  | C-3 |
B636 | 4 |  | B-3 |  | J/C
B637 | 4 |  | B-3 |
：White or natural color

WIRING SYSTEM > Engine Wiring Harness
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
E3 | 76 |  | B-5 | B139 | Bulkhead wiring harness
E4 | 2 | B | B-3 |  | Purge control solenoid valve
E5 | 2 | Gr | B-2 |  | Fuel injector No. 1
E6 | 2 | Gr | B-3 |  | Fuel injector No. 3
E10 | 3 | B | B-4 |  | Crankshaft position sensor
E11 | 1 |  | C-3 |  | Oil pressure switch
E14 | 2 | B | B-3 |  | Knock sensor 1
E16 | 2 | Gr | C-4 |  | Fuel injector No. 2
E17 | 2 | Gr | C-4 |  | Fuel injector No. 4
E18 | 6 | Gr | B-3 |  | EGR control valve
E21 | 3 | B | B-3 |  | Manifold absolute pressure sensor
E31 | 3 | B | B-2 |  | Ignition coil No. 1
E32 | 3 | B | C-4 |  | Ignition coil No. 2
E33 | 3 | B | B-2 |  | Ignition coil No. 3
E34 | 3 | B | C-4 |  | Ignition coil No. 4
E35 | 3 | Gr | C-4 |  | Intake camshaft position sensor LH
E36 | 3 | Gr | B-2 |  | Intake camshaft position sensor RH
E37 | 2 | B | C-4 |  | Intake oil control solenoid LH
E38 | 2 | B | B-1 |  | Intake oil control solenoid RH
E48 | 2 | B | B-4 |  | Knock sensor 2
E51 | 5 | Gr | B-5 |  | Tumble generator valve actuator LH
E55 | 5 | Gr | B-3 |  | Tumble generator valve actuator RH
E57 | 6 | B | B-4 |  | Electronic throttle control
E62 | 3 | Gr | C-1 |  | Exhaust camshaft position sensor RH
E63 | 2 | B | B-1 |  | Exhaust oil control solenoid RH
E65 | 3 | Gr | C-4 |  | Exhaust camshaft position sensor LH
E66 | 2 | B | C-4 |  | Exhaust oil control solenoid LH
E75 | 2 | B | C-3 |  | Engine oil temperature sensor
E115 | 30 | B | B-4 | T15 | Transmission cord
E127 | 11 | Gr | B-4 | F135 | Front wiring harness
E130 | 1 |  | C-3 |  | Oil level switch
E158 | 114 | B | B-5 |  | ECM
E160 | 2 | B | C-4 |  | High-pressure fuel pump
E162 | 4 | B | B-3 |  | Fuel pressure sensor
E164 | 5 | Gr | B-4 |  | Thermo control valve ASSY
E165 | 2 | Gr | B-3 | E166 | Adapter cord (knock sensor 1)
E166 | 2 | Gr | B-3 | E165 | Engine wiring harness
E167 | 2 | Gr | B-4 | E168 | Adapter cord (knock sensor 2)
E168 | 2 | Gr | B-4 | E167 | Engine wiring harness
E169 | 2 | Gr | B-4 | E170 | Adapter cord (fuel injector No. 4)
E170 | 2 | Gr | B-4 | E169 | Engine wiring harness
E171 | 2 | B | C-3 |  | Engine coolant temperature sensor (INLET)
E172 | 2 | B | B-3 |  | Engine coolant temperature sensor (OUTLET)
GE-1 | ― | ― | B-4 |  | ―
：White or natural color

WIRING SYSTEM > Transmission Cord
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AT1 | 3 | B | B-4 |  | Primary speed sensor
AT4 | 3 | Gr | C-4 |  | Secondary speed sensor
AT5 | 3 | Gr | C-3 |  | Turbine speed sensor
AT6 | 3 | B | C-4 |  | Secondary pressure sensor
T7 | 9 | B | B-3 |  | Inhibitor switch
T10 | 48 | B | B-3 |  | TCM
T11 | 10 |  | B-2 |  | Control valve body
T15 | 30 | B | B-2 | E115 | Engine wiring harness
T27 | 4 | B | C-4 |  | Electric fluid pump
GT-1 | ― | ― | B-3 |  | ―
GT-2 | ― | ― | C-4 |
：White or natural color

WIRING SYSTEM > Instrument Panel Wiring Harness RH
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB6 | 45 | Y | B-1 |  | Airbag CM
AB9 | 4 | Y | A-3 |  | Passenger's airbag module
AB27 | 2 | Y | A-3 |
AD15 | 4 | B | C-4 |  | Audio/Navigation unit
AD16 | 4 | B | D-4 |  | AUX input terminal (instrument panel)
AD26 | 22 |  | D-2 | i287 | Instrument panel wiring harness
AD27 | 8 |  | C-2 |  | Front seat heater switch
AD28 | 2 |  | C-2 |  | Shift position indicator (without shift position pointer)
4 |  | C-2 |  | Shift position indicator (with shift position pointer)
AD30 | 4 | Gr | C-2 |  | X MODE switch
AD64 | 22 | Gr | D-2 |  | J/C
AD67 | 10 |  | C-2 |  | AVH/EPB control switch
AD71 | 2 |  | D-3 | i149 | Instrument panel wiring harness
AD72 | 8 |  | D-3 |  | USB power supply (console)
AD77 | 4 | B | C-4 |  | Audio/Navigation unit
AD78 | 4 | Br | C-4 |  | Data communication module
i21 | 18 |  | A-3 |  | J/C
i23 | 2 |  | B-3 |  | Glove box illumi. light
i24 | 2 | B | D-5 |  | Front accessory power supply socket
i29 | 1 | B | C-4 |  | Audio case ground
i33 | 5 |  | B-2 |  | ID code box
i34 | 16 |  | B-2 |  | Immobilizer CM
i44 | 8 |  | C-1 |  | Select lever
i46 | 2 | B | D-3 |  | Rear accessory power supply socket (console)
i51 | 2 |  | A-1 |  | Sunload sensor
i71 | 3 |  | C-2 |  | Keyless access interior antenna (front)
i76 | 46 |  | B-3 | D83 | Front door cord RH
i85 | 10 |  | C-5 |  | Audio/Navigation unit
i87 | 28 |  | C-4 |
i88 | 40 |  | D-5 |  | A/C control panel
i89 | 3 |  | A-3 |  | Auto light sensor
i122 | 12 | B | A-1 |  | MFD (with standard MFD)
24 |  | A-1 |  | MFD (with high grade MFD)
i131 | 6 |  | C-5 |  | Audio/Navigation unit
i146 | 5 |  | D-4 |
i149 | 2 |  | D-3 | AD71 | Adapter cord (USB power supply (console) )
i159 | 4 |  | A-3 |  | Side tweeter RH
i163 | 10 |  | C-2 |  | AVH/EPB control switch
i164 | 2 |  | D-4 |  | OP connector (power amplifier)
i168 | 4 |  | A-3 |  | J/C
i169 | 4 |  | A-3 |
i172 | 2 | Br | A-2 |  | Evaporator sensor
i174 | 6 | B | D-5 |  | Air mix door actuator (without L/R independent air conditioner)
6 | B | D-5 |  | Air mix door actuator RH (with L/R independent air conditioner)
i183 | 6 | B | B-2 |  | Power transistor
i184 | 4 |  | B-3 |  | Blower motor relay
i185 | 2 |  | B-2 |  | Blower motor
i218 | 2 |  | B-3 | i290 | Short connector
i259 | 2 |  | D-5 |  | Pocket light
i270 | 20 | Gr | C-4 |  | Data communication module
i271 | 16 | Gr | C-4 |
i282 | 64 |  | B-3 | R464 | Rear wiring harness RH
i283 | 48 |  | B-3 | R465
i287 | 22 |  | D-2 | AD26 | Adapter cord (console)
i290 | 2 |  | B-3 | i218 | Short connector
i291 | 6 |  | B-3 |  | OP connector (remote engine start CM) (with push button start)
i293 | 2 |  | B-2 |  | Heater core sensor
i294 | 6 | B | A-2 |  | Intake door actuator
i295 | 8 |  | D-4 |  | AUX input terminal (instrument panel)
i297 | 22 | B | A-1 |  | J/C
i298 | 22 | B | A-2 |
i313 | 10 |  | D-4 |  | Door lock back up unit
i343 | 4 |  | D-5 |  | J/C
i344 | 2 | B | D-3 | R140 | Adapter cord (rear brake caliper RH)
i345 | 2 |  | D-3 | R149 | Adapter cord (rear brake caliper LH)
i347 | 8 |  | A-1 |  | Driver monitoring unit
i350 | 2 |  | C-2 |  | Shift position indicator
GB-2 | ― | ― | B-3 |  | ―
GB-3 | ― | ― | B-1 |
：White or natural color

WIRING SYSTEM > Instrument Panel Wiring Harness LH
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB2 | 4 | Y | C-4 |  | Roll connector
AB35 | 2 |  | D-4 |  | F/B
AB66 | 2 | B | C-3 |  | Driver's knee airbag module
AB75 | 2 |  | C-1 | i302 | Short connector
i5 | 16 | L | D-4 |  | F/B
i10 | 40 | B | A-4 |  | Combination meter
i19 | 14 |  | A-1 | R96 | Roof cord
i28 | 4 |  | C-2 |  | OP connector (fog light switch)
i47 | 7 | B | B-4 |  | Steering lock CM
i52 | 2 | B | B-4 |  | Key lock solenoid
i58 | 8 |  | B-4 |  | Ignition switch
i60 | 5 |  | C-4 |  | Immobilizer antenna
i63 | 2 |  | C-5 |  | Key warning switch
i68 | 7 |  | B-5 |  | Combination switch
i69 | 10 |  | B-4 |
i72 | 14 |  | C-4 |  | Roll connector
i73 | 20 |  | B-4 |  | Combination switch
i74 | 5 |  | C-4 |  | Steering angle sensor
i75 | 28 |  | B-3 |  | Keyless access CM
i79 | 6 |  | C-2 |  | Illumination control switch
i81 | 32 | B | D-5 |  | Body integrated unit
i82 | 18 |  | B-2 |  | J/C
i84 | 10 |  | D-5 |  | Body integrated unit
i94 | 8 | L | C-2 |  | BSD/RCTA OFF switch
i101 | 46 |  | C-1 | D84 | Front door cord LH
i112 | 86 |  | B-2 | B60 | Bulkhead wiring harness
i115 | 4 | Y | B-2 | B49
i136 | 40 | Gr | D-4 |  | F/B
i137 | 12 | Br | D-4 |
i140 | 4 |  | A-1 |  | J/C
i141 | 4 |  | A-1 |
i150 | 14 | B | B-5 |  | Push button ignition switch
i157 | 22 |  | A-1 | R50 | Roof cord
i158 | 4 |  | A-2 |  | Side tweeter LH
i166 | 4 |  | B-2 |  | J/C
i167 | 4 |  | B-2 |
i171 | 40 |  | D-5 |  | Body integrated unit
i173 | 4 |  | B-5 |  | In-vehicle sensor
i175 | 6 | B | B-4 |  | Air mix door actuator LH
i176 | 6 | B | B-4 |  | Mode door actuator
i215 | 18 |  | B-2 | B129 | Bulkhead wiring harness
i216 | 6 |  | B-2 | B130
i234 | 8 | B | C-2 |  | VDC OFF switch
i236 | 8 | Gr | C-2 |  | Auto Start Stop cancel switch
i241 | 30 |  | A-3 |  | Keyless access CM
i257 | 4 |  | C-2 |  | Memory height switch
i258 | 4 | Gr | C-2 |  | Power rear gate driver's switch
i265 | 8 |  | D-4 |  | F/B
i266 | 12 |  | D-4 |
i267 | 2 |  | B-3 |  | Trip switch
i275 | 22 | B | B-4 |  | J/C
i277 | 4 | Gr | C-2 |  | SRH OFF switch
i280 | 5 | Gr | B-2 |  | Steering heater/Seat heater relay
i284 | 64 |  | D-2 | R466 | Rear wiring harness LH
i285 | 48 |  | D-1 | R467
i288 | 16 |  | C-3 |  | Data link connector
i289 | 4 |  | C-4 |  | Roll connector
i291 | 6 |  | C-4 |  | OP connector (remote engine start CM) (without push button start)
i302 | 2 |  | C-1 | AB75 | Short connector
i315 | 8 | B | B-2 |  | Fuse holder
i346 | 8 | G | C-2 |  | Driver monitoring system OFF switch
i352 | 4 |  | B-2 |  | J/C
i353 | 4 |  | B-2 |
GB-4 | ― | ― | D-1 |  | ―
：White or natural color

WIRING SYSTEM > Steering Wheel Cord
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB37 | 2 | Or | C-3 |  | Driver's airbag module
AB38 | 2 | B | C-3 |
ST3 | 12 |  | B-3 |  | Roll connector
ST4 | 4 |  | B-3 |
ST5 | 4 |  | C-2 |  | Steering switch
ST8 | 4 |  | C-4 |  | Steering heater switch
ST9 | 3 |  | C-4 |
ST10 | 5 |  | C-3 |  | Steering heater CM
ST11 | 4 |  | B-3 | ST12 | Roll connector
ST12 | 4 |  | B-3 | ST11 | Satellite switch (without steering heater)
4 |  | B-3 | ST11 | Steering heater harness (with steering heater)
ST14 | 4 |  | C-3 |  | Steering heater CM
ST15 | — |  | C-4 |  | Horn switch
：White or natural color

WIRING SYSTEM > Roof Cord
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
R50 | 22 |  | D-3 | i157 | Instrument panel wiring harness
R51 | 2 | B | A-1 |  | Vanity mirror light RH
R52 | 3 |  | A-3 |  | Room light (without sunroof)
3 |  | A-4 |  | Room light (with sunroof)
R54 | 2 | B | B-3 |  | Vanity mirror light LH
R55 | 10 | Gr | A-3 |  | Sunroof unit
R96 | 14 |  | C-3 | i19 | Instrument panel wiring harness
R128 | 5 |  | B-2 |  | Sunroof switch (slide)
R137 | 16 |  | B-2 |  | Stereo camera
R139 | 5 |  | A-2 |  | OP connector (rearview mirror)
R161 | 5 |  | B-2 |  | Warning box
R288 | 4 |  | B-3 |  | J/C
R405 | 16 |  | A-2 | R407 | Adapter cord (stereo camera cover)
16 |  | A-2 | R407 | Adapter cord (overhead console)
R406 | 6 | Gr | A-2 |  | Pre-collision brake OFF & lane departure warning OFF switch
R407 | 16 |  | A-2 | R405 | Roof cord
R463 | 8 |  | B-2 |  | Telematics button
：White or natural color

WIRING SYSTEM > Rear Wiring Harness RH
LOCATION
1. FRONT

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB18 | 45 | Y | D-3 |  | Airbag CM
AB24 | 2 | Y | C-4 |  | Side airbag module RH
AB25 | 2 | Y | C-4 | AB43 | Seat position sensor harness
AB26 | 2 | B | A-4 |  | Seat belt pretensioner RH
AB28 | 2 | B | A-4 |  | Side impact sensor RH (center pillar)
AB30 | 2 | Or | B-4 |  | Lap belt pretensioner RH
AB53 | 6 | Gr | B-4 | AB59 | Occupant detection wiring harness
AB82 | 2 | B | A-4 |  | Adaptive belt RH
R12 | 4 | Gr | A-4 |  | Front door switch RH
R13 | 12 |  | A-4 | D28 | Rear door cord RH
R82 | 18 |  | C-4 | R81 | Rear wiring harness LH
R124 | 2 | Y | C-1 | AB63 | Front door cord RH
R315 | 30 |  | C-4 |  | Audio amplifier
R316 | 24 |  | C-4 |
R334 | 14 |  | B-4 | R349 | Adapter cord (front seat RH)
R464 | 64 |  | C-1 | i282 | Instrument panel wiring harness
R465 | 48 |  | C-1 | i283
GB-6 | ― | ― | C-3 |  | ―
：White or natural color

2. REAR

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB33 | 2 | B | A-1 |  | Curtain airbag module RH
AB34 | 2 | B | B-3 |  | Side impact sensor RH (rear wheel house)
AB68 | 4 | Y | A-4 |  | Rear seat belt pretensioner RH
R16 | 4 | Gr | B-3 |  | Rear door switch RH
R26 | 4 | Gr | A-5 |  | Rear combination light RH
R49 | 14 |  | A-4 |  | Rear seat heater CM
R53 | 16 | B | A-4 |
R58 | 6 | Gr | D-2 |  | Fuel pump ASSY
R61 | 10 | B | B-5 |  | Radar sensor RH (slave)
R70 | 6 |  | D-2 |  | Rear seat heater (seat cushion)
R72 | 2 | Gr | C-3 |  | Rear ABS wheel speed sensor RH
R97 | 1 |  | A-5 | AN8 | Antenna cord
R117 | 4 |  | A-5 |  | Woofer
R170 | 8 |  | C-3 |  | Remote control back rest RH
R172 | 5 |  | A-5 |  | Remote control back rest switch RH
R261 | 4 |  | A-4 |  | Fuel lid lock actuator
R266 | 4 |  | A-5 | R267 | Short connector
R267 | 4 |  | A-5 | R266
R297 | 3 |  | D-4 |  | Keyless access interior antenna (center)
R298 | 3 |  | D-5 |  | Keyless access interior antenna (rear)
R400 | 8 | Gr | D-4 |  | Leak check valve ASSY
R492 | 2 | Gr | B-5 |  | Keyless access exterior antenna (rear)
GB-5 | ― | ― | A-5 |  | ―
：White or natural color

WIRING SYSTEM > Rear Wiring Harness LH
LOCATION
1. FRONT

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB17 | 45 | Y | C-1 |  | Airbag CM
AB19 | 2 | Y | B-3 |  | Side airbag module LH
AB21 | 2 | B | B-4 |  | Seat belt pretensioner LH
AB23 | 2 | B | B-4 |  | Side impact sensor LH (center pillar)
AB29 | 2 | Or | C-4 |  | Lap belt pretensioner LH
AB41 | 2 | B | A-3 |  | Side impact sensor (under the rear center seat)
AB74 | 2 | Y | C-3 | AB83 | Seat position sensor harness
AB81 | 2 | B | B-4 |  | Adaptive belt LH
AD68 | 14 |  | B-2 | R138 | Rear wiring harness LH
AD69 | 8 | Be | A-3 |  | Rear seat heater switch LH
AD70 | 6 |  | A-3 |  | Rear seat heater switch RH
R9 | 4 | Gr | B-4 |  | Front door switch LH
R10 | 12 |  | B-5 | D22 | Rear door cord LH
R59 | 4 | Gr | A-4 |  | Fuel sub level sensor
R81 | 18 |  | B-2 | R82 | Rear wiring harness RH
R108 | 2 |  | B-3 |  | Front seat belt switch LH (without power seat)
R123 | 2 | Y | D-2 | AB62 | Front door cord LH
R138 | 14 |  | B-2 | AD68 | Adapter cord (rear seat heater switch)
R341 | 14 |  | B-3 | R205 | Adapter cord (front seat LH)
R361 | 24 |  | C-3 |  | RAB CM
R466 | 64 |  | D-2 | i284 | Instrument panel wiring harness
R467 | 48 |  | D-2 | i285
R489 | 32 |  | B-3 | R505 | Adapter cord (power seat & remote control mirror CM)
R490 | 14 |  | D-2 | D163 | Front door cord LH
GB-8 | ― | ― | C-2 |  | ―
：White or natural color

2. REAR

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB31 | 2 | B | C-1 |  | Curtain airbag module LH
AB32 | 2 | B | C-3 |  | Side impact sensor LH (rear wheel house)
AB67 | 4 | Y | C-3 |  | Rear seat belt pretensioner LH
R22 | 4 | Gr | D-3 |  | Rear door switch LH
R25 | 10 | B | C-5 |  | Radar sensor LH (master)
R28 | 4 | Gr | B-5 |  | Rear combination light LH
R32 | 2 | B | B-4 |  | Rear accessory power supply socket (cargo room)
R38 | 18 |  | A-2 | D34 | Rear gate cord (UPR)
R39 | 11 |  | A-2 | D35
R73 | 2 | Gr | D-3 |  | Rear ABS wheel speed sensor LH
R79 | 8 |  | C-5 |  | OP connector (trailer)
R80 | 12 |  | B-4 |  | Keyless entry CM
R141 | 3 |  | A-2 |  | Luggage room light
R171 | 8 |  | D-2 |  | Remote control back rest LH
R173 | 5 |  | B-4 |  | Remote control back rest switch LH
R180 | 22 | B | D-2 |  | J/C
R207 | 4 |  | B-5 | R208 | Short connector
R208 | 4 |  | B-5 | R207
R211 | 12 |  | B-4 |  | TPMS CM
R221 | 12 |  | B-4 |  | TPMS & keyless entry CM
R362 | 10 | B | B-5 | R368 | Sonar sensor cord
R422 | 16 | B | B-4 |  | Power rear gate CM
R423 | 6 | B | B-4 |
R424 | 14 | Gr | C-4 |
R486 | 8 |  | B-4 |  | Power rear gate drive unit
GB-7 | ― | ― | C-4 |  | ―
：White or natural color

WIRING SYSTEM > Front Seat Wiring Harness RH
LOCATION
1. MANUAL SEAT

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB43 | 2 | Y | C-3 | AB25 | Rear wiring harness RH
AB44 | 2 | B | D-3 |  | Seat position sensor RH
AB59 | 6 | Gr | C-3 | AB53 | Rear wiring harness RH
AB60 | 2 | Y | C-3 |  | Buckle switch (RH)
AB61 | 12 | B | C-4 |  | Occupant detection CM
AB69 | 12 | Gr | C-4 |
AB70 | 3 | B | C-4 |  | Load sensor 1 (FL)
AB71 | 3 | Gr | C-3 |  | Load sensor 3 (RL)
AB72 | 3 | Gr | D-3 |  | Load sensor 2 (FR)
AB73 | 3 | B | C-2 |  | Load sensor 4 (RR)
R349 | 14 |  | C-3 | R334 | Rear wiring harness RH
R471 | 2 | G | C-3 | R472 | FB heater
R472 | 2 | G | C-3 | R471 | FC heater
：White or natural color

2. POWER SEAT

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB43 | 2 | Y | C-3 | AB25 | Rear wiring harness RH
AB44 | 2 | B | D-3 |  | Seat position sensor RH
AB59 | 6 | Gr | C-3 | AB53 | Rear wiring harness RH
AB60 | 2 | Y | C-3 |  | Buckle switch (RH)
AB61 | 12 | B | C-3 |  | Occupant detection CM
AB69 | 12 | Gr | C-3 |
AB70 | 3 | B | C-4 |  | Load sensor 1 (FL)
AB71 | 3 | Gr | C-3 |  | Load sensor 3 (RL)
AB72 | 3 | Gr | D-3 |  | Load sensor 2 (FR)
AB73 | 3 | B | C-2 |  | Load sensor 4 (RR)
R190 | 10 |  | D-3 |  | Power seat switch RH
R191 | 6 |  | B-3 |  | Reclining motor
R192 | 5 | Gr | D-4 |  | Slide motor
R193 | 6 |  | C-4 |  | Tilt motor
R194 | 6 |  | C-2 |  | Lifter motor
R349 | 14 |  | C-3 | R334 | Rear wiring harness RH
R378 | 14 |  | C-3 | R379 | Front seat heater RH
R379 | 14 |  | C-3 | R378 | Adapter cord (front seat RH)
R413 | 2 | Gr | C-3 | R414 | Adapter cord (reclining motor)
R414 | 2 | Gr | C-3 | R413 | Adapter cord (front seat RH)
R471 | 2 | G | C-3 | R472 | FB heater
R472 | 2 | G | C-3 | R471 | FC heater
：White or natural color

WIRING SYSTEM > Front Seat Wiring Harness LH
LOCATION
1. MANUAL SEAT

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB83 | 2 | Y | C-3 | AB74 | Rear wiring harness LH
AB84 | 2 | B | D-3 |  | Seat position sensor LH
R205 | 14 |  | C-3 | R341 | Rear wiring harness LH
R469 | 2 | G | C-3 | R470 | FB heater
R470 | 2 | G | C-3 | R469 | FC heater
：White or natural color

2. POWER SEAT WITHOUT SEAT POSITION MEMORY

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB83 | 2 | Y | C-3 | AB74 | Rear wiring harness LH
AB84 | 2 | B | D-3 |  | Seat position sensor LH
R108 | 2 |  | C-3 |  | Front seat belt switch LH
R196 | 2 |  | C-3 | R197 | Adapter cord (lumbar motor)
R197 | 2 |  | C-3 | R196 | Adapter cord (front seat LH)
R198 | 2 |  | C-4 |  | Lumbar motor
R200 | 18 |  | D-3 |  | Power seat switch LH
R201 | 6 |  | B-3 |  | Reclining motor
R202 | 5 | Gr | D-2 |  | Slide motor
R203 | 6 |  | C-2 |  | Tilt motor
R204 | 6 |  | C-4 |  | Lifter motor
R205 | 14 |  | C-3 | R341 | Rear wiring harness LH
R380 | 14 |  | C-3 | R381 | Front seat heater LH
R381 | 14 |  | C-3 | R380 | Adapter cord (front seat LH)
R411 | 2 | Gr | C-3 | R412 | Adapter cord (reclining motor)
R412 | 2 | Gr | C-3 | R411 | Adapter cord (front seat LH)
R469 | 2 | G | C-3 | R470 | FB heater
R470 | 2 | G | C-3 | R469 | FC heater
：White or natural color

3. POWER SEAT WITH SEAT POSITION MEMORY

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB83 | 2 | Y | C-3 | AB74 | Rear wiring harness LH
AB84 | 2 | B | D-3 |  | Seat position sensor LH
R108 | 2 |  | C-3 |  | Front seat belt switch LH
R196 | 2 |  | C-3 | R197 | Adapter cord (lumbar motor)
R197 | 2 |  | C-3 | R196 | Adapter cord (front seat LH)
R198 | 2 |  | C-4 |  | Lumbar motor
R200 | 18 |  | D-3 |  | Power seat switch LH
R201 | 6 |  | B-3 |  | Reclining motor
R202 | 5 | Gr | D-2 |  | Slide motor
R203 | 6 |  | C-2 |  | Tilt motor
R204 | 6 |  | C-4 |  | Lifter motor
R205 | 14 |  | C-3 | R341 | Rear wiring harness LH
R380 | 14 |  | C-3 | R381 | Front seat heater LH
R381 | 14 |  | C-3 | R380 | Adapter cord (front seat LH)
R411 | 5 | Gr | C-3 | R412 | Adapter cord (reclining motor)
R412 | 5 | Gr | C-3 | R411 | Adapter cord (front seat LH)
R469 | 2 | G | C-3 | R470 | FB heater
R470 | 2 | G | C-3 | R469 | FC heater
R502 | 30 |  | C-2 |  | Power seat & remote control mirror CM
R503 | 24 |  | C-2 |
R504 | 26 |  | C-3 |
R505 | 32 |  | C-2 | R489 | Rear wiring harness LH
：White or natural color

WIRING SYSTEM > Door Cord RH
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB63 | 2 | Y | C-1 | R124 | Rear wiring harness RH
AB64 | 2 | B | B-2 |  | Side impact sensor RH (front door)
D12 | 2 |  | C-2 |  | Front door speaker RH
D13 | 2 | B | C-2 |  | Front power window motor RH (with driver's seat only off delay function)
8 | B | C-2 |  | Front power window motor RH (with front seats only off delay function)
D15 | 16 |  | B-2 |  | Outer mirror ASSY RH (without seat position memory)
24 |  | B-2 |  | Outer mirror ASSY RH (with seat position memory)
D17 | 5 |  | B-2 |  | Front power window sub-switch (with driver's seat only off delay function)
8 | Gr | B-2 |  | Front power window sub-switch (with front seats only off delay function)
D18 | 10 |  | B-3 |  | Front door lock actuator RH
D20 | 2 |  | C-3 |  | Front door step light RH
D28 | 12 |  | B-4 | R13 | Rear wiring harness RH
D29 | 2 |  | B-4 |  | Rear door speaker RH
D30 | 2 | B | B-4 |  | Rear power window motor RH (without telematics)
8 | B | B-4 |  | Rear power window motor RH (with telematics)
D31 | 5 |  | B-4 |  | Rear power window switch RH (without telematics)
8 | Gr | B-4 |  | Rear power window switch RH (with telematics)
D32 | 10 |  | A-5 |  | Rear door lock actuator RH
D56 | 6 |  | B-3 |  | Outer handle RH
D83 | 46 |  | C-1 | i76 | Instrument panel wiring harness
D125 | 8 |  | B-2 |  | Passenger's door lock switch
：White or natural color

WIRING SYSTEM > Door Cord LH
LOCATION

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AB58 | 2 | B | C-4 |  | Side impact sensor LH (front door)
AB62 | 2 | Y | D-5 | R123 | Rear wiring harness LH
D2 | 2 |  | C-4 |  | Front door speaker LH
D3 | 8 | B | D-4 |  | Front power window motor LH
D5 | 16 |  | C-4 |  | Outer mirror ASSY LH (without seat position memory)
24 |  | C-4 |  | Outer mirror ASSY LH (with seat position memory)
D7 | 16 | B | C-4 |  | Power window main switch
D10 | 2 |  | C-3 |  | Front door step light LH
D22 | 12 |  | C-2 | R10 | Rear wiring harness LH
D23 | 2 |  | C-2 |  | Rear door speaker LH
D24 | 2 | B | C-2 |  | Rear power window motor LH (without telematics)
8 | B | C-2 |  | Rear power window motor LH (with telematics)
D25 | 5 |  | B-1 |  | Rear power window switch LH (without telematics)
8 | Gr | B-1 |  | Rear power window switch LH (with telematics)
D26 | 10 |  | B-1 |  | Rear door lock actuator LH
D66 | 6 |  | B-3 |  | Outer handle LH
D72 | 10 |  | B-3 |  | Front door lock actuator LH
D84 | 46 |  | D-5 | i101 | Instrument panel wiring harness
D143 | 8 |  | C-4 |  | Seat position memory switch
D149 | 24 |  | C-4 |  | Remote control mirror switch
D163 | 14 |  | D-5 | R490 | Rear wiring harness LH
：White or natural color

WIRING SYSTEM > Rear Wiring Harness and Rear Gate Cord
LOCATION

Connector | Connecting to |  |
No. | Pole | Color | Area | No. | Description |  |
D34 | 18 |  | A-2 | R38 | Rear wiring harness LH |  |
D35 | 11 |  | A-2 | R39 |  |
D39 | 2 |  | A-3 |  | High-mounted stop light |  |
D43 | 4 |  | B-4 |  | Rear wiper motor |  |
D44 | 2 |  | B-4 |  | License plate light RH |  |
D46 | 4 |  | C-3 |  | Rear gate lock actuator & latch switch |  |
D47 | 2 | Br | B-4 |  | Rear gate opener button |  |
D48 | 1 | B | B-2 |  | Rear defogger |  |
D77 | 4 |  | B-4 |  | Rear lock button & rear gate opener button |  |
D80 | 18 |  | C-3 | D81 | Rear gate cord (LWR) |  |
D81 | 18 |  | C-3 | D80 | Rear gate cord (UPR) |  |
D85 | 4 |  | C-3 |  | Rearview camera |  |
D87 | 4 |  | B-5 |  | Rear finisher light RH |  |
D89 | 1 | B | B-5 |  | Rear defogger |  |
D91 | 4 |  | C-2 |  | Rear finisher light LH |  |
D137 | 2 |  | C-3 |  | License plate light LH |  |
D150 | 2 |  | B-4 |  | Power rear gate touch sensor RH |  |
D151 | 2 |  | C-2 |  | Power rear gate touch sensor LH |  |
D152 | 2 | Gr | C-4 |  | Power rear gate buzzer |  |
D153 | 8 |  | C-3 |  | Power rear gate auto closer |  |
D154 | 4 | Gr | C-4 |  | Power rear gate inner switch |  |
D155 | 11 |  | C-3 | D156 | Rear gate cord (LWR) |  |
D156 | 11 |  | C-3 | D155 | Rear gate cord (UPR) |  |
D161 | 3 |  | C-3 |  | Rear gate light |  |
D162 | 4 |  | C-4 |  | Power rear gate lock button |  |
R140 | 2 | Gr | B-1 | i344 | Instrument panel wiring harness |  |
R149 | 2 | Gr | B-1 | i345 |  |
R153 | 2 | B | C-4 |  | Rear brake caliper RH |  |
R154 | 2 | B | C-1 |  | Rear brake caliper LH |  |
R364 | 2 | B | D-2 |  | Sonar sensor (left corner) |  |
R365 | 2 | B | D-3 |  | Sonar sensor (left inner) |  |
R366 | 2 | B | C-5 |  | Sonar sensor (right corner) |  |
R367 | 2 | B | C-4 |  | Sonar sensor (right inner) |  |
R368 | 10 | B | D-2 | R362 | Rear wiring harness LH |  |
GB-11 | ― | ― | C-2 |  | ― |  |
：White or natural color |  |

WIRING SYSTEM > Antenna Cord
LOCATION
1. FRONT

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AN1 | 3 |  | C-3 |  | Audio/Navigation unit
AN2 | 1 | L | C-2 |
AN3 | 3 |  | B-5 | AN4 | Antenna cord (without telematics)
3 | L | B-5 | AN4 | Antenna cord (with telematics)
AN4 | 3 |  | B-5 | AN3 | Antenna cord (without telematics)
3 | L | B-5 | AN3 | Antenna cord (with telematics)
AN9 | 1 | Gr | C-2 |  | Audio/Navigation unit
AN10 | 1 | G | B-1 |  | GPS antenna (without navigation)
2 |  | B-1 |  | GPS antenna (with navigation)
AN11 | 1 | G | C-3 |  | Data communication module
AN12 | 1 | Gr | C-3 |
AN13 | 1 | Br | C-3 |
：White or natural color

2. REAR

Connector | Connecting to
No. | Pole | Color | Area | No. | Description
AN5 | 3 |  | B-4 | AN6 | Antenna cord (without telematics)
3 | L | B-4 | AN6 | Antenna cord (with telematics)
AN6 | 3 |  | B-4 | AN5 | Antenna cord (without telematics)
3 | L | B-4 | AN5 | Antenna cord (with telematics)
AN7 | 3 | Gr | B-3 |  | Antenna
AN8 | 1 |  | C-4 | R97 | Rear wiring harness RH
AN14 | 1 | V | B-3 |  | Telematics antenna
：White or natural color