( TL19E00D52100063635KDAT00 )

VSA Modulator-control Unit Removal and Installation

NOTE:

- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid gets on the paint, wash it off immediately with water.
- Be careful not to damage or deform the brake lines during removal and installation.
- Plug the end of a hose and joints to prevent spilling brake fluid.

Removal

1. Turn the ignition switch to LOCK (0).

1. Remove the suction line mount bolt (A) from the bracket.

1. Disconnect the receiver line (B) from the clamp (C).