( TL19E20A20326428001KAAT00 )

Fuel Line/Quick-Connect Fitting Removal

1. To prevent damage and keep foreign matter out, cover the disconnected connector and line ends with plastic bags (A).
   NOTE: The retainer cannot be reused once it has been removed from the line.
   Replace the retainer when:
   - replacing the fuel rail.
   - replacing the fuel line.
   - replacing the fuel pump.
   - replacing the fuel filter.
   - replacing the fuel tank.
   - it has been removed from the line.
   - it is damaged.