( TL19E20A18313200000LAAT00 )

Balancer Shaft/Balancer Shaft Holder Assembly Overhaul

1. Apply new engine oil to the threads of the balancer shaft sprocket mounting bolt (A).

1. Loosely install the balancer shaft/balancer shaft holder assembly (B) with new O-rings (C), then install the balancer shaft sprocket (D).

1. Remove the pin driver (E), then tighten the balancer shaft/balancer shaft holder assembly mounting bolts.

1. Tighten the chain guide mounting bolt (F).