( TL19E00J2622021929CKDAT00 )

Dashboard Center Trim Removal/Installation

NOTE:

- Take care not to scratch the trim and panels.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Remove these items:
   - Center console panel
   - Passenger's side: Passenger's dashboard trim

1. Remove the driver's center trim (A) or the passenger's center trim (B).

   -1. | Remove the screw(s) (C).
   -2. | Gently pull the lower portion of the trim up to detach the clip (D) and to release the hook (E) from the edge of the center console (F).
   -3. | Pull out the trim to detach the clips (G, H).

1. Install the trim in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.

Driver's side
Passenger's side