( TL19E1AE34100000000HAAT07 )

Hard to shift into reverse

Probable cause(s)

1. Worn or incorrect MTF.
2. Clutch defective.
3. Reverse shift fork defective.
4. Reverse idler gear defective.
5. Reverse gear defective.
6. Change lever assembly defective.

Diagnostic procedure

- Check and/or replace the MTF.
- Check the clutch.
- Check the reverse shift fork.
- Check the reverse idler gear.
- Check reverse gear.
- Check the change lever assembly.