( TL19E00J26220219291KDAT00 )

Dashboard Center Panel Removal/Installation

Without Audio System
NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trims tool or equivalent.

1. Remove these items:
   - Center console panel
   - Driver's center trim
   - Passenger's dashboard trim
   - Passenger's center trim
   - Center holder
   - Climate control unit
   - Center pocket

1. Pull out the center panel (A) by hand to detach the clips, and disconnect the hazard warning switch connector (B), then remove the panel.

1. Install the panel in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Make sure the hazard warning switch connector is plugged in properly.
   - Push the clips into place securely.