( TL19E00J10300000000FAAT06 )

Audio System Symptom Troubleshooting - No sound is heard from the speaker(s) (display is normal) (without premium audio system)

1. Check the resistance between the following terminals of audio unit connector A (24P) according to the table.

   Speaker | Terminal | Wire color
   --- | --- | ---
   Left front door speaker, Left front door tweeter | A23 (+) | LT GRN
   A22 (−) | PNK
   Right front door speaker, Right front door tweeter | A19 (+) | GRY
   A18 (−) | RED
   Left rear speaker | A11 (+) | YEL
   A10 (−) | BRN
   Right rear speaker | A7 (+) | BLU
   A6 (−) | ORN

Is there continuity?

YES | - | Go to Step 11 .
NO | - | Repair an open in the wires between the audio unit and speaker(s).■

1. Disconnect the speaker 2P connector.