( TL19E00J10300000000FAAT02 )

Audio System Symptom Troubleshooting - Poor AM or FM radio reception or interference (without premium audio system)

1. Measure the voltage between the AM/FM antenna 3P connector terminal No. 3 and body ground.

Is there battery voltage?

YES | - | Go to Step 15 .
NO | - | Go to Step 10 .

1. Turn the ignition switch to LOCK (0).

1. Remove the audio unit.

1. Disconnect audio unit connector E (3P).