( TL19E00J26200031201KDAT00 )

Headliner Removal/Installation

1. Lower the headliner (A).

   -1. | Remove the front door opening seals (B) and rear door opening seals (C) from each roof portion.
   -2. | With the help of an assistant, detach the rear clips (D) by pulling the rear portion of the headliner down.
   -3. | With sunroof: Detach the front clips (E) and the Velcro fasteners (F) by lowering the sunroof opening edge of the headliner.

Without sunroof
With sunroof