( TL19E00K75100081070FAAT00 )

DTC Troubleshooting: 7, 13

1. Check for continuity between LKAS control unit 26P connector No. 25 terminal and VSA modulator-control unit 47P connector No. 13 terminal.

Is there continuity?

YES | - | Check for loose terminals in the VSA modulator-control unit connector, and repair if necessary. If all connections are OK, replace the VSA modulator-control unit. ■
NO | - | Repair an open in the wire between the LKAS control unit and the branch of the F-CAN line (CANL).■