( TL19E00D14300014751KBAT00 )

Brake Hose Replacement

NOTE:

- Before reassembling, check that all parts are free of dirt and other foreign particles.
- Replace parts with new ones whenever specified to do so.
- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid gets on the paint, wash it off immediately with water.
- Plug the end of a hose and joints to prevent spilling brake fluid.

Front
NOTE: The illustrations show the 1-piston caliper type.

1. Remove the front wheel.

1. Disconnect the brake line (A) from the brake hose (B), then remove the brake hose clip (C).