( TL19E00J32133100000FAAT00 )

HID Lamp System Troubleshooting

1. Remove the bulb, and check the luminescence part of the HID bulb.

Is there black discoloration or transformation?

YES | - | Replace the HID bulb(s), and recheck, then go to Step 15 .
NO | - | Go to Step 9 .

1. Substitute the right and left HID bulbs.

Does the symptom change to the other side?

YES | - | Replace the HID bulb and recheck, then go to Step 15 .
NO | - | Go to Step 10 .

1. Turn the combination light switch OFF.

1. Disconnect the HID unit 2P connector.

1. Turn the combination light (headlight) switch ON.