( TL19E000000000K3031BAAT00 )

Service Reminder System General Information - for applicable EU countries

Resetting the Service Reminder Information Display
NOTE:

- The vehicle must be stopped to reset the display.
- If a required service is done and the display is not reset, or if the service reminder information display is reset without doing the service the system will not show the proper maintenance timing. This can lead to serious mechanical problems because there will be no accurate record of when the required maintenance is needed.
- Each maintenance item can be independently reset with the HDS.

1. Turn the ignition switch to ON (II).

1. Press the SEL/RESET switch repeatedly until the service reminder information display appears.

1. Press and hold the SEL/RESET button for about 10 seconds, the service reminder reset display appears.
   NOTE:
   - If you are resetting the display when the remaining days are more than30 days, make sure any maintenance item(s) requiring service are done before resetting the display.
   - To cancel the reset mode, push the SEL/RESET switch.