( TL19E00D52100000000FAAT05 )

VSA System Symptom Troubleshooting - ABS indicator, brake system indicator, VSA indicator, and TSA warning do not go off at the same time

1. Check for continuity between VSA modulator-control unit 47P connector terminal No. 16 and body ground.

Is there continuity?

YES | - | Go to Step 17 .
NO | - | Repair open in the wire between the VSA modulator-control unit and body ground (G202).■

1. Disconnect the gauge control module 32P connector.