( TL19E00J54200014401KDAT00 )

Battery Removal/Installation

NOTE: The battery terminal disconnection/reconnection procedure must be done before and after doing this procedure. Some systems store data in memory that is lost when the battery is disconnected.
Removal

1. Do the battery terminal disconnection procedure.

1. Remove the two nuts (A) securing the battery setting plate, then remove the battery setting plate (B), battery cover (C) and the battery (D).