( TL19E00K77C000Y2625FAAT00 )

DTC Troubleshooting: B2625

1. Check for continuity between the left front corner parking sensor 6P connector No. 4 terminal and body ground.

Is there continuity?

YES | - | Repair a short to ground in the wire.■
NO | - | Go to Step 19 .

1. Reconnect all connectors.

1. Turn the ignition switch to ON (II).

1. Check for DTCs with the HDS.

Is DTC B2628 also indicated?

YES | - | Go to the DTC B2628 troubleshooting.■
NO | - | Replace the parking and back-up sensor control unit .■