( TL19E00J34600000000CAAT00 )

Entry Lights Control System (Ceiling Lights, Map Lights, Ignition Key Light)
The driver's MICU controls the interior lights ON/OFF based upon the input signals from each switch.

| Input | Output
--- | --- | ---
Driver's MICU | IG1 power supply Ignition key switch Driver's door switch Left [right] rear door switch | Interior lights Ignition key light
B-CAN | Keyless LOCK/UNLOCK signal Front passenger's door switch Right [left] rear door switch Driver's door lock knob switch (LOCK/UNLOCK) |

[ ]: | RHD model